This information is subject to change without notice.See Notice of Disclaimer on Title Page.3-1593.3National ISDN-2 PRI SolutionsThe guides in Section 3.3 use the capabilities of the National ISDN-2 Primary Rate Interface (PRI).This interface is comprised of 23 B channels and one D channel and is sometimes designated "23B +D." Like the BRI, each PRI B channel is 64 kbps. The D channel in PRI also operates at 64 kbps, isused for signaling only, and is not used for user data. The bandwidth of the PRI allows it to provideaccess to a variety of network services by customer premises equipmentNI-2 provides the following capabilities on Primary Rate Interfaces:¥Call-by-Call Service Selection - allows private network users to specify a network service to beused by a B channel call. This feature is necessary because unlike non-ISDN trunks, PRI allowsseveral services to be provided over a single trunk. Examples of services which may be specifiedinclude non-ISDN Foreign Exchange (FX) facilities, non-ISDN Tie Trunks, Inward Wide AreaTelecommunications Service (INWATS), Outward Wide Area Telecommunications Service(OUTWATS), and access to Electronic Tandem Networks (ETNs).¥Calling Number Identification Services for PRI - allows network users to control thedelivery/privacy of Calling and Redirecting Numbers.¥SWF-DS1 (Switched Fractional DS1) or Multirate ISDN - allows a user to establish and clearcalls through a PRI at rates of N x 64 kbps, where N = 2 to 24. The case where N=6 (384 kbps) isknown as an H0 channel, and the case where N=24 (1536 kbps) is known as an H11 channel.¥Interworking with Private Networks - allows a PRI to be used as a tie trunk in private networksto connect two Private Branch Exchanges (PBXs), two Centrex switches, or one PBX and oneCentrex switch.The nine application groups covered are listed in the table below, followed by the numbers of theindividual guides that belong to each group.LANSSCREENSHARINGVIDEOVOICE&DATAFILETRANSFERWORK-AT-HOMEFAX &IMAGETRANS-ACTIONSOTHER

3.3.13.3.53.3.93.3.123.3.14

3.3.23.3.63.3.103.3.133.3.15

3.3.33.3.73.3.113.3.16

3.3.43.3.83.3.17

This information is subject to change without noticeSee Notice of Disclaimer on Title Page3-160