This information is subject to change without notice.See Notice of Disclaimer on Title Page4-89894.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

AT&T7506VoiceOne Channel

263 Sherman Blvd.Circuit-DataOne Channel

Naperville, IL 60566-7050B Channel PacketNo

Don Ziemann(708) 713-7039D Channel PacketYes

NI-1 Date:NowPrice: contact distributor for current priceSimultaneous activecallsOne Voice &One Data

NI-2 Date:1994FCC Class:Uses 1 DN or 2?One

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display 2 x 24Async¥ V.120Yes, 38.4X.25 Term. SupportYes

Speaker Phone?Yes¥ OtherDMI 57.6Async PADYes

Feature Keys?17SynchSync PAD

Analog Interface¥ V.120¥ Other Logical Channels

Data Interface RS-232B CHANNEL PACKET

ISDN Interface S/T56/64 kbps YesX.25 Term. SupportNo

Power Interface PS1 & PS 2112/128 kbpsAsync PAD

Self-Initializing?YesBonding?Sync PAD

NIIGs: 2,3,4,6,7,8,21Stores CallingNumber? Yes Logical Channels

NIPGs: 1,2,3,4,5,7Dialing AT&T CMD,Modes: Hayes ATAPIs Supported:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-9090Additional Features:¥ Includes 2 x24 display with 17 programmable call appearance and feature keys¥ Includes message waiting lamp and a speaker phone and personalized ringing¥ Includes self test and line diagnostics¥ Supports AT&T CMD command set and the AT command set and an Application Programming Interface¥ Supports asynchronous data up to 57.6 Kbps¥ Includes PAD for D channel Packet Mode calls¥ Supports V. 120 and DMI Modes 2 & 3 rate adaption and will provide automatic selection for incoming CMD or PMD calls.

4.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

AT&T7507VoiceOne Channel

263 Sherman Blvd.Circuit-DataOne Channel

Naperville, IL 60566-7050B Channel PacketNo

Don Ziemann(708) 713-7039D Channel PacketYes

NI-1 Date:NowPrice: contact distributor for current priceSimultaneous activecallsOne Voice &One Data

NI-2 Date:1994FCC Class:Uses 1 DN or 2?One

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display 2 x 40Async¥ V.120Yes, 38.4X.25 Term. SupportYes

Speaker Phone?Yes¥ OtherDMI 57.6Async PADYes

Feature Keys?17SynchSync PAD

Analog Interface¥ V.120¥ Other Logical Channels

Data Interface RS-232B CHANNEL PACKET

ISDN Interface S/T56/64 kbps YesX.25 Term. SupportNo

Power Interface PS1 or PS 2112/128 kbpsAsync PAD

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-9191Self-Initializing?YesBonding?Sync PAD

NIIGs: 2,3,4,6,7,8,21Stores CallingNumber? Yes Logical Channels

NIPGs: 1,2,3,4,5,7Dialing AT&T CMD,Modes: Hayes ATAPIs Supported:

Additional Features:¥ Includes 2 x40 display with 39 programmable call appearance and feature keys¥ Includes message waiting lamp and a speaker phone and personalized ringing¥ Includes self test and line diagnostics¥ Supports AT&T CMD command set and the AT command set and an Application Programming Interface¥ Supports asynchronous data up to 57.6 Kbps¥ Includes PAD for D channel Packet Mode calls¥ Supports V. 120 and DMI Modes 2 & 3 rate adaption and will provide automatic selection for incoming CMD or PMD calls.

4.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Cortelco, Inc.CortelcoVoiceOne Channel

4119 Willow Lake Blvd.30 ButtonISDN SetCircuit-DataOne Channel

Memphis, TN 38118B Channel PacketNo

Mary S. Towey(901) 365-7774D Channel PacketYes

NI-1 Date:NowPrice:Simultaneous activecallsOne Voice &One Data

NI-2 Date:First Q’94FCC Class:BUses 1 DN or 2?Two

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display2 x 24 or 4 x 40Async¥ V.120 YesX.25 Term. SupportYes

Speaker Phone?Yes¥ Other T-LinkAsync PAD

Feature Keys?30/78SynchSync PADYes

Analog InterfaceNo¥ V.120Yes¥ Other Logical Channels

Data Interface RS-232/V.35B CHANNEL PACKET

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-9292ISDN Interface S/T & U56/64 kbps YesX.25 Term. SupportNo

Power InterfacePS 2112/128 kbps NoAsync PAD

Self-Initializing?YesBonding? NoSync PAD

NIIGs:1-13Stores CallingNumber? Yes Logical Channels

NIPGs:1-7DialingModes:APIs Supported:

Additional Features:¥ 30 button models with optional 48 add on button module¥ Self initializing; speed dial; speaker phone with group listen; date & time; display incoming call info; auto answer; local speed dial; Hot Dial Pad;¥ Integrated NT-1 with 30 button set¥ Data package now available¥ Supports all NI-1 terminal modes¥ 2 x 24 or 4 x 40 display

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-93934.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Cortelco, Inc.CortelcoVoiceOne Channel

4119 Willow Lake Blvd.18 ButtonISDN SetCircuit-DataOne Channel

Memphis, TN 38118B Channel PacketNo

Mary S. Towey(901) 365-7774D Channel PacketYes

NI-1 Date:NowPrice:Simultaneous activecallsOne Voice &One Data

NI-2 Date:First Q’94FCC Class:BUses 1 DN or 2?Two

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display 2 x 24Async¥ V.120YesYesX.25 Term. SupportYes

Speaker Phone?Yes¥ OtherT-LinkAsync PAD

Feature Keys?18/64SynchSync PADYes

Analog InterfaceNo¥ V.120Yes¥ Other Logical Channels

Data Interface RS-232/V.35B CHANNEL PACKET

ISDN Interface S/T56/64 kbpsYesX.25 Term. SupportNo

Power InterfacePS 2112/128 kbpsAsync PAD

Self-Initializing?YesBonding?NoSync PAD

NIIGs:1-13Stores CallingNumber?Yes Logical Channels

NIPGs:1-7Dialing Modes:APIs Supported:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-9494Additional Features:¥ 18 and 30 button models with optional 48 add on button module¥ Self initializing; speed dial; speaker phone with group listen; date & time; display incoming call info; auto answer; 2 x 24; locally programmed speed dials; Hot Dial Pad;¥ Data package now available¥ Supports all NI-1 terminal modes

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-95954.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

FujitsuSRS 1050VoiceYes

ISDN Division4403 Bland RoadCircuit-DataYes

Somerset ParkRaleigh, NC 27609B Channel PacketNo

Ann Daly(919) 790 - 2032D Channel PacketYes

NI-1 Date:NowPrice:Simultaneous activecalls2

NI-2 Date:Planned*FCC Class:BUses 1 DN or 2?2

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

DisplayYesAsync¥ V.120Yes38.4X.25 Term. SupportYes

Speaker Phone?Yes¥ OtherAsync PADYes

Feature Keys?18Sync PAD

Analog InterfaceNoSynchN/A Logical Channels1

Data InterfaceRS-232¥ V.120¥ OtherB CHANNEL PACKETN/A

ISDN InterfaceS/T56/64 kbpsYesX.25 Term. Support

Power InterfaceNT1- 7&8 (P2)AC option available112/128 kbpsNoAsync PAD

Self-Initializing?YesBonding?NoSync PAD

NIIGs: 1-4,6,7,8,10,11,12,14, 15,17,20,21,22,24,25,27Stores Calling Number? Yes (8) Logical Channels

NIPGs: #1-8Dialing Stored, keypad,Modes: keyboardAPIs Supported:None

Additional Features:CartridgeUpgradeData LED IndicatorsCall LogData LoopbackSoft KeysQ.931 Message LoggingPrinter Pinfeed Templates Available (and associated PC printing program)*As specifications are available

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-96964.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

FujitsuSRS 2000VoiceYes

ISDN Division4403 Bland RoadCircuit-DataYes,

Somerset ParkRaleigh, NC 27609B Channel PacketNo

Ann Daly(919) 790 - 2032D Channel PacketYes

NI-1 Date:NowPrice:Simultaneous activecalls5ESS - two ,DMS - one

NI-2 Date:Planned*FCC Class:AUses 1 DN or 2?1

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

DisplayYesAsync¥ V.120Yes19.2X.25 Term. SupportYes

Speaker Phone?Yes¥ OtherV.110Async PADYes

Feature Keys?32Sync PADNo

Analog InterfaceNoSynch Logical Channels1

Data InterfaceRS-232¥ V.120¥ OtherV.110 19.2B CHANNEL PACKETN/A

ISDN InterfaceS/T56/64 kbpsYesX.25 Term. Support

Power InterfaceNT1- 7&8 (P2)AC option available112/128 kbpsNoAsync PAD

Self-Initializing?Layer 1 & 2 Yes SPID Yes; SPM NoBonding?NoSync PAD

NIIGs: 1-4,6,7,8,10,11,12,14, 15,17,20,21,22,24,25,27Stores Calling Number? Yes (8) Logical Channels

NIPGs: #1-8Dialing Stored, keypadModes: keyboardAPIs Supported:None

Additional Features:CartridgeUpgradeData LED IndicatorsCall LogData LoopbackSoft KeysQ.931 Message LoggingData Module added/changed w/only 2 screwsPrinter Pinfeed Templates Available (and associated PC printing program)*As soon as specifications are available

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-97974.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Lodestar Technology, Inc.LT1-2002UVoiceYes (30+ Callappearances)

3101 MaGuire Blvd., Suite 251Orlando, FL 32803Circuit-DataOne Channel

(407) 895-0881B Channel PacketNo

FAX (407) 895-3566D Channel PacketYes

NI-1 Date:NowPrice:Simultaneous activecalls30

NI-2 Date:NowFCC Class:BUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display40 x 4Async¥ V.120Yes, 38.4 KbpsX.25 Term. Support

Speaker Phone?Yes¥ OtherAsync PADYes

Feature Keys?35Analog InterfaceNoSynch¥ V.120¥ OtherYes, 64 KbpsSync PAD Logical Channels1

Data Interface RS-232 V.24 Sync56/64 kbpsBothB CHANNEL PACKET

ISDN Interface U112/128 kbpsX.25 Term. SupportAsync PAD

Power Interface 7.5 V DCBondingSync PAD

Self-Initializing?YesStores Calling Number? Yes Logical Channels

NIIGs: 1,2,3,4,6,7,8,10,11,12, 20,21,22NIPGs: 1,2,3,4,5,7Dialing Enbloc andModes: overlap sendingAPIs Supported:Hayes AT for bothdata ports. PADfor D-packet

Additional Features:¥ Two data ports¥ Automatic switch type detection and adaption to AT&T and NTI pre NI-1 or after NI-1 releases.¥ Battery backup (rechargeable) up to 3 hours.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-9898

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-99994.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Lodestar Technology, Inc.LT1-2002SVoiceYes (30+ Call Appearances)

3101 MaGuire Blvd., Suite 251Orlando, FL 32803Circuit-DataOne Channel

(407) 895-0881B Channel PacketNo

FAX (407) 895-3566D Channel PacketYes

NI-1 Date:NowPrice:Simultaneous activecalls30

NI-2 Date:NowFCC Class:BUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display40 x 4Async¥ V.120Yes, 38.4 KbpsX.25 Term. Support

Speaker Phone?Yes¥ OtherAsync PADYes

Feature Keys?35Sync PAD

Analog InterfaceNoSynch Logical Channels1

Data Interface RS-232, V.24 Sync¥ V.120¥ Other Yes, 64 KbpsB CHANNEL PACKET

ISDN Interface S/TX.25 Term. Support

Power Interface PS 2 and external power adapter of 48 V DC56/64 kbps112/128 kbpsBothAsync PAD

Self-Initializing?YesBonding?Sync PAD

NIIGs: 1,2,3,4,6,7,8,10,11,12, 20,21,22Stores Calling Number? Logical Channels

NIPGs: 1,2,3,4,5,7Dialing Enbloc andModes: overlap sendingAPIs Supported:Hayes AT for both dataports PAD for D-packet

Additional Features:¥ Two data ports¥ Automatic detection and adaption of switch types such as AT&T 5ESS and NTI’s DMS-100¥ Battery backup (rechargeable) up to 3 hours.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-100100

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1011014.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Lodestar Technology, Inc.LT1-1501UVoiceYes (10 Call Appearances)

3101 MaGuire Blvd., Suite 251Orlando, FL 32803Circuit-DataOne Channel

(407) 895-0881B Channel PacketNo

FAX (407) 895-3566D Channel PacketYes

NI-1 Date:NowPrice:Simultaneous activecalls10

NI-2 Date:NowFCC Class:BUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display24 x 2Async¥ V.120Yes, 37.6 KbpsX.25 Term. Support

Speaker Phone?Yes¥ OtherAsync PADYes

Feature Keys?10Sync PAD

Analog InterfaceNoSynch Logical Channels1

Data Interface RS-232¥ V.120¥ Other Yes, 64 KbpsB CHANNEL PACKET

ISDN Interface UX.25 Term. Support

Power Interface 7.5 V DC External56/64 kbps112/128 kbpsBothAsync PAD

Self-Initializing?YesBonding?Sync PAD

NIIGs: 1,2,3,4,6,7,8,10,11,12, 20,21,22Stores CallingNumber?Yes Logical Channels

NIPGs: 1,2,3,4,5,7DialingModes:APIs Supported:

Additional Features:¥ Automatic detection and adaption to AT&T and NTI’s various switch types¥ Battery backup (rechargeable) up to 3 hours.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1021024.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Lodestar Technology, Inc.LT1-1501SVoiceYes (10 Call Appearances)

3101 MaGuire Blvd., Suite 251Orlando, FL 32803Circuit-DataOne Channel

(407) 895-0881B Channel PacketNo

FAX (407) 895-3566D Channel PacketYes

NI-1 Date:September, 1993Price:Simultaneous activecalls10

NI-2 Date:September, 1993FCC Class:BUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display24 x 2Async¥ V.120Yes, 37.6 KbpsX.25 Term. Support

Speaker Phone?Yes¥ OtherAsync PADYes

Feature Keys?10Sync PAD

Analog InterfaceNoSynch Logical Channels1

Data Interface RS-232¥ V.120¥ Other Yes, 64 KbpsB CHANNEL PACKET

ISDN Interface S/TX.25 Term. Support

Power Interface PS 2, and external, phantom56/64 kbps112/128 kbpsBothAsync PAD

Self-Initializing?YesBonding?Sync PAD

NIIGs: 1,2,3,4,6,7,8,10,11,12, 20,21,22Stores CallingNumber?Yes Logical Channels

NIPGs: 1,2,3,4,5,7Dialing Enbloc andModes: overlap sendingAPIs Supported:

Additional Features:¥ Automatic detection and adaption to AT&T and NTI’s various switch types¥ Battery backup (rechargeable) up to 3 hours.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1031034.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Lodestar Technology, Inc.LT1-1001SVoiceYes (10 Call Appearances)

3101 MaGuire Blvd., Suite 251Orlando, FL 32803Circuit-DataNo

(407) 895-0881B Channel PacketNo

FAX (407) 895-3566D Channel PacketNo

NI-1 Date:October, 1993Price:Simultaneous activecalls10

NI-2 Date:October, 1993FCC Class:BUses 1 DN or 2?One

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

DisplayOption of 16 x 1Async¥ V.120X.25 Term. Support

Speaker Phone?Yes¥ OtherAsync PADNo

Feature Keys?YesNoSync PAD

Analog InterfaceNoSynch Logical Channels1

Data Interface No¥ V.120¥ OtherB CHANNEL PACKET

ISDN Interface S/TX.25 Term. Support

Power Interface phantom, PS 256/64 kbps112/128 kbpsAsync PADNo

Self-Initializing?YesBonding?Sync PAD

NIIGs: 2Stores CallingNumber? Logical Channels

NIPGs: 1,2,3,4,5DialingModes:APIs Supported:

Additional Features:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1041044.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Lodestar Technology, Inc.LT1-1001UVoiceYes (10 Call Appearances)

3101 MaGuire Blvd., Suite 251Orlando, FL 32803Circuit-DataNo

(407) 895-0881B Channel PacketNo

FAX (407) 895-3566D Channel PacketNo

NI-1 Date:October, 1993Price:Simultaneous activecalls10

NI-2 Date:October, 1993FCC Class:BUses 1 DN or 2?One

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

DisplayOption of 16 x 1Async¥ V.120X.25 Term. Support

Speaker Phone?Yes¥ OtherAsync PADNo

Feature Keys?YesNoSync PAD

Analog InterfaceNoSynch Logical Channels1

Data Interface No¥ V.120¥ OtherB CHANNEL PACKET

ISDN Interface UX.25 Term. Support

Power Interface External, 7.5 V DC56/64 kbps112/128 kbpsAsync PADNo

Self-Initializing?YesBonding?Sync PAD

NIIGs: 2Stores CallingNumber? Logical Channels

NIPGs: 1,2,3,4,5DialingModes:APIs Supported:

Additional Features:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1051054.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Motorola UDSVDS 120VoiceYes

5000 Bradford DriveHuntsville, AL 35805Circuit-DataYes

Dean SharpB Channel PacketNo

(205) 430-8902D Channel PacketYes

NI-1 Date:May 1994Price:TBASimultaneous activecallsTwo

NI-2 Date:FCC Class:AUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display2 x 24Async¥ V.120Yes, 57.6X.25 Term. SupportNo

Speaker Phone?Yes¥ OtherT-Link, 19.2Async PADYes

Feature Keys?28Sync PADNo

Analog InterfaceNoSynch Logical Channels1

Data Interface RS-232¥ V.120¥ OtherYes, 19.2T-Link, 64KB CHANNEL PACKET

ISDN InterfaceS/TX.25 Term. Support

Power Interface AC, PS-1, PS-256/64 kbps112/128 kbpsYesNoAsync PAD

Self-Initializing?YesBonding?NoSync PAD

NIIGs: 1,2,3,6,7,11,21Stores CallingNumber?Yes Logical Channels

NIPGs: 1,2,3,4,5,6,7DialingKeypad, AT,Modes:V.25 bis, DTRAPIs Supported:

Additional Features:¥ Remote configuration¥ Software download option

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1061064.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Northern Telecom, Inc.M5317TDXVoiceOne Channel

4001 E. Chapel Hill-NelsonHwyCircuit-DataOne Channel

Research Triangle Park, NC27709B Channel PacketNo

Bill Barnhill(919) 255-8946FAX: (919) 992-6548D Channel PacketSimultaneous activecallsYesOne Voice,One Data

NI-1 Date:7/1/93Price: $675

NI-2 Date:FCC Class:AUses 1 DN or 2?Two

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display 2 x 40Async¥ V.12019.2 KX.25 Term. Support19.2K

Speaker Phone? Yes¥ Other T-Link19.2KAsync PAD19.2K

Feature Keys? 12 Hard, 5 SoftSync PADNo

Analog Interface NoSynch Logical ChannelsOne

Data Interface RS-232C DB25¥ V.120¥ OtherNoB CHANNEL PACKET

ISDN Interface S/TX.25 Term. Support

Power Interface PS1, PS256/64 kbpsNoAsync PAD

Self-Initializing? Yes112/128 kbpsNoSync PAD

NIIGs:Bonding?No Logical Channels

NIPGs:Stores CallingNumber? YesAPIs Supported:Hayes Extended ATX.28

DialingModes:Extended AT X.28

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-107107Additional Features:NI-1 BELLCORE Tested

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1081084.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Northern Telecom, Inc.M5209TVoiceOne Channel

4001 E. Chapel Hill-NelsonHwyCircuit-DataOne Channel

Research Triangle Park, NC27709B Channel PacketNo

Bill Barnhill(919) 255-8946FAX: (919) 992-6548D Channel PacketSimultaneous activecallsYesOne Voice,One Data

NI-1 Date:4/1/93Price: $580

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display 2 x 24Async¥ V.12038.4KX.25 Term. Support9.6K

Speaker Phone? Speaker, No Microphone¥ Other T-Link19.2KAsync PAD9.6K

Feature Keys? 9Sync PADNo

Analog Interface NoSynch Logical ChannelsOne

Data Interface RS-232C DB25¥ V.120¥ OtherNoB CHANNEL PACKET

ISDN Interface S/TX.25 Term. Support

Power Interface PS256/64 kbpsNoAsync PAD

Self-Initializing? Yes112/128 kbpsNoSync PAD

NIIGs:Bonding?No Logical Channels

NIPGs:Stores CallingNumber? YesAPIs Supported:Hayes Extended ATX.3, X.28

DialingModes:Extended AT X.28

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-109109Additional Features:NI-1 BELLCORE Tested

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1101104.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Siemens Stromberg-CarlsonSSC-ISDN SET 782VoiceOne Channel

900 Broken Sound ParkwayACDCircuit-DataOne Channel

Boca Raton, FL 33487ANSI & NI-1Compatible TerminalB Channel PacketNone

Dan Bonner(407) 955-3037D Channel PacketNo

NI-1 Date:NowPrice:Simultaneous activecallsTwo; one voice &one data

NI-2 Date:FCC Class:Uses 1 DN or 2?One or more

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 24Async¥ V.120Yes - 19.2 KbpsX.25 Term. Support

Speaker Phone? Yes¥ OtherDMi-2 - 19.2 KbpsAsync PAD

Feature Keys? Yes; 16/32Sync PAD

Analog Interface NSynch Logical Channels

Data Interface RS-232¥ V.120¥ OtherB CHANNEL PACKET

ISDN Interface S/TX.25 Term. Support

Power Interface Line PS1 or PS256/64 kbps112/128 kbpsYesNoAsync PAD

Self-Initializing? YesBonding?NoSync PAD

NIIGs: 2-4, 6-8, 11, 12, 15Stores CallingNumber?Yes Logical Channels

NIPGs: 1-6DialingModes: Hayes ATAPIs Supported:

Additional Features:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1111114.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Siemens Stromberg-CarlsonSSC-ISDN SET 787VoiceOne or TwoChannels

900 Broken Sound ParkwayBoca Raton, FL 33487ANSI & NI-1Compatible TerminalCircuit-DataOne Channel

Dan BonnerB Channel PacketNone

(407) 955-3037D Channel PacketNo

NI-1 Date:NowPrice:Simultaneous activecallsTwo; one/twovoice &/or onedata

NI-2 Date:FCC Class:Uses 1 DN or 2?One or more

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 24Async¥ V.120Yes - 19.2 KbpsX.25 Term. Support

Speaker Phone? Yes¥ Other DMI-2 - 19.2 KbpsAsync PAD

Feature Keys? Yes; 16/32Sync PAD

Analog Interface NoSynch Logical Channels

Data Interface RS-232¥ V.120¥ OtherB CHANNEL PACKET

ISDN Interface S/TX.25 Term. Support

Power Interface Line PS1 or PS256/64 kbps112/128 kbpsYesNoAsync PAD

Self-Initializing? YesBonding?NoSync PAD

NIIGs: 2-4, 6-8, 11, 12, 15Stores CallingNumber?Yes Logical Channels

NIPGs: 1-6DialingModes: Hayes ATAPIs Supported:

Additional Features:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1121124.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Telrad CommunicationsIDS - 284/VVoiceOne Channel

135 Crossways Park DriveCircuit-DataNone

Woodbury, NY 11797B Channel PacketNone

Erv Sloan(516) 921-8300D Channel PacketNone

NI-1 Date:NowPrice:Simultaneous activecallsOne voice

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?One

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 24Async¥ V.120 NoX.25 Term. SupportNo

Speaker Phone? Speaker - no microphone¥ OtherAsync PADNo

Feature Keys?Yes; 10Sync PADNo

Analog InterfaceNoSynch Logical Channels

Data Interface ¥ V.120¥ Other: NoB CHANNEL PACKET

ISDN Interface S/TX.25 Term. SupportN/A

Power Interface PS1; PS2; External56/64 kbps112/128 kbps NoAsync PAD

Self-Initializing?YesBonding? NoSync PAD

NIIGs: 2, 4, 6Stores CallingNumber?TBA Logical Channels

NIPGs: 1-5Dialing Modes: Speed Dial;Key PAD; Last NumberRedial: Save & RepeatAPIs Supported:

Additional Features:¥ Multiple CO configurations; DMS Custom: 5ESS Custom; NI1 are part of the software and called into use form the Man-Machine interface. No cartridges are required.¥

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1131134.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Telrad CommunicationsIDS - 284/PVoiceOne Channel

135 Crossways Park DriveCircuit-DataNone

Woodbury, NY 11797B Channel PacketNone

Erv Sloan(516) 921-8300D Channel PacketYes

NI-1 Date:NowPrice:Simultaneous activecallsTwo; one voice &one data PAD

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 24Async¥ V.120NoX.25 Term. SupportNo

Speaker Phone? Speaker - no microphone¥ OtherAsync PADYes; 9600

Feature Keys?Yes; 10Sync PADNo

Analog InterfaceNoSynch Logical Channels1

Data Interface RS-232, V.24¥ V.120¥ Other: NoB CHANNEL PACKET

ISDN Interface S/TX.25 Term. SupportN/A

Power Interface PS1; PS2; External56/64 kbps112/128 kbpsNoNoAsync PAD

Self-Initializing?YesBonding?NoSync PAD

NIIGs: 2, 4, 6, 8, 20, 25, 27Stores CallingNumber?TBA Logical Channels

NIPGs: 1-5, 7-8Dialing Modes: Auto Ans &Orig. Keypad; Dialing;Power On; MnemonicsAPIs Supported:

Additional Features:¥ Multiple CO configurations; including DMS and 5ESS Custom capability are part of the set software and called into use form the Man-Machine interface. No cartridges are required.¥ Field Upgradable from 284/V

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1141144.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Telrad CommunicationsIDS - 284/D1VoiceOne Channel

135 Crossways Park DriveCircuit-DataOne Channel

Woodbury, NY 11797B Channel PacketNone

Erv Sloan(516) 921-8300D Channel PacketYes

NI-1 Date:NowPrice:Simultaneous activecallsTwo; one voice &one data (B or D)

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 24Async¥ V.120Yes - 38.4 KbpsX.25 Term. SupportNo

Speaker Phone? Speaker - no microphone¥ Other DMi - 19.2 KbpsT-link - 19.2 KbpsTelrad - 38.4 KbpsAsync PADYes; 9600

Feature Keys?Yes; 10Sync PADNo

Analog InterfaceNoSynch Logical Channels1

Data Interface RS-232, V.24¥ V.120¥ Other: NoB CHANNEL PACKET

ISDN Interface S/T¥ DMI - 56/64 Kbps¥ T-Link - 56/64 Kbps¥ Telrad - 56/64 KbpsX.25 Term. SupportN/A

Power Interface PS1; PS2; External56/64 kbps112/128 kbpsYesNoAsync PAD

Self-Initializing?YesBonding?NoSync PAD

NIIGs: 2-4, 6-8, 11, 12, 15, 17, 21, 22, 25, 27Stores CallingNumber?TBA Logical Channels

NIPGs: 1-5, 7-8Dialing Modes: Auto Ans &Orig. Hayes AT; ExtendedHayes; Keypad; SpeedDialing; Power On;MnemonicsAPIs Supported:Hayes AT;Extended AT

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-115115Additional Features:¥ Multiple CO configurations; Rate adaption schemes and SYNC/ASYNC capability are part of the set software and called into use from the Man-Machine interface No cartridges are required.¥ D-channel messages and commands can be sent/received through the RS-232 data port. Useful for Call Management applications.¥ Field Upgradable from 284/V

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1161164.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Telrad CommunicationsIDS - 285/VVoiceOne Channel

135 Crossways Park DriveCircuit-DataNone

Woodbury, NY 11797B Channel PacketNone

Erv Sloan(516) 921-8300D Channel PacketNone

NI-1 Date:NowPrice:Simultaneous activecallsOne voice

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?One

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 24Async¥ V.120NoX.25 Term. SupportNo

Speaker Phone? Yes¥ OtherAsync PADNo

Feature Keys?Yes; 10Sync PADNo

Analog InterfaceNoSynch Logical Channels

Data Interface ¥ V.120¥ Other: NoB CHANNEL PACKET

ISDN Interface S/TX.25 Term. SupportN/A

Power Interface PS1; PS2; External56/64 kbps112/128 kbpsNoAsync PAD

Self-Initializing?YesBonding?NoSync PAD

NIIGs: 2, 4, 6Stores CallingNumber?TBA Logical Channels

NIPGs: 1-5Dialing Modes: Speed Dial;Key PAD; Last NumberRedial; Save and RepeatAPIs Supported:

Additional Features:¥ Multiple CO configurations; DMS Custom; 5ESS Custom; NI1 are part of the software and called into use from the Man-Machine interface. No cartridges are required.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1171174.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Telrad CommunicationsIDS - 285/PVoiceOne Channel

135 Crossways Park DriveCircuit-DataNone

Woodbury, NY 11797B Channel PacketNone

Erv Sloan(516) 921-8300D Channel PacketYes

NI-1 Date:NowPrice:Simultaneous activecallsTwo; One Voice &One PMD

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 24Async¥ V.120NoX.25 Term. SupportNo

Speaker Phone? Yes¥ OtherAsync PADYes; 9600

Feature Keys?Yes; 10Sync PADNo

Analog InterfaceNoSynch Logical Channels1

Data Interface RS-232, V.24¥ V.120¥ Other: NoB CHANNEL PACKET

ISDN Interface S/TX.25 Term. SupportN/A

Power Interface PS1; PS2; External56/64 kbps112/128 kbpsNoNoAsync PAD

Self-Initializing?YesBonding?NoSync PAD

NIIGs: 2, 4, 6, 8, 20, 25, 27Stores CallingNumber?TBA Logical Channels

NIPGs: 1-5, 7-8Dialing Modes: Auto Ans &Orig. Keypad; Dialing;Power On; MnemonicsAPIs Supported:Hayes AT;Extended AT

Additional Features:¥ Multiple CO configurations; including DMS and 5ESS Custom capability are part of the set software and called into use from the Man-Machine interface. No cartridges are required.¥ Field Upgradable from 285/V

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1181184.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Telrad CommunicationsIDS - 285/D1VoiceOne Channel

135 Crossways Park DriveCircuit-DataOne Channel

Woodbury, NY 11797B Channel PacketNone

Erv Sloan(516) 921-8300D Channel PacketYes

NI-1 Date:NowPrice:Simultaneous activecallsTwo; one voice &one data (B or D)

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 24Async¥ V.120Yes - 38.4 KbpsX.25 Term. SupportNo

Speaker Phone? Yes¥ Other DMI - 19.2 KbpsT-link - 19.2 KbpsTelrad - 38.4 KbpsAsync PADYes; 9600

Feature Keys?Yes; 10Sync PADNo

Analog InterfaceNoSynch Logical Channels1

Data Interface RS-232, V.24¥ V.120¥ Other: NoB CHANNEL PACKET

ISDN Interface S/T¥ DMI - 56/64 Kbps¥ T-Link - 56/64 Kbps¥ Telrad - 56/64 KbpsX.25 Term. SupportN/A

Power Interface PS1; PS2; External56/64 kbps112/128 kbpsYesNoAsync PAD

Self-Initializing?YesBonding?NoSync PAD

NIIGs: 2-4, 6-8, 10, 11, 12, 17, 21, 22, 25, 27Stores CallingNumber?TBA Logical Channels

NIPGs: 1-5, 7-8Dialing Modes: Auto Ans &Orig. Hayes AT; ExtendedHayes; Keypad; SpeedDialing; Power On;MnemonicsAPIs Supported:Hayes AT;Extended AT

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-119119Additional Features:¥ Multiple CO configurations; Rate adaption schemes and SYNC/ASYNC capability are part of the set software and called into use from the Man-Machine interface No cartridges are required.¥ D-channel messages and commands can be sent/received through the RS-232 data port. Useful for Call Management applications.¥ Field Upgradable from 285/V

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1201204.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Telrad CommunicationsIDS - 286/VVoiceOne Channel

135 Crossways Park DriveCircuit-DataNone

Woodbury, NY 11797B Channel PacketNone

Erv Sloan(516) 921-8300D Channel PacketNone

NI-1 Date:NowPrice:Simultaneous activecallsOne voice

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?One

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 24Async¥ V.120 NoX.25 Term. Support

Speaker Phone? Yes¥ OtherAsync PAD

Feature Keys?Yes; 16Sync PAD

Analog InterfaceNoSynch Logical Channels

Data Interface ¥ V.120¥ Other: NoB CHANNEL PACKET

ISDN Interface S/TX.25 Term. SupportN/A

Power Interface PS1; PS2; External56/64 kbps112/128 kbps NoAsync PAD

Self-Initializing?YesBonding? NoSync PAD

NIIGs: 2, 4, 6Stores CallingNumber?TBA Logical Channels

NIPGs: 1-5Dialing Modes:APIs Supported:

Additional Features:¥ Multiple CO configurations; DMS Custom; 5ESS Custom, NI1 are part of the software and called into use from the Man-Machine interface. No cartridges are required.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1211214.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Telrad CommunicationsIDS - 286/PVoiceOne Channel

135 Crossways Park DriveCircuit-DataNone

Woodbury, NY 11797B Channel PacketNone

Erv Sloan(516) 921-8300D Channel PacketYes

NI-1 Date:NowPrice:Simultaneous activecallsTwo; one voice &one PMD

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 24Async¥ V.120NoX.25 Term. SupportNo

Speaker Phone? Yes¥ OtherAsync PADYes; 9600

Feature Keys?Yes; 16Sync PADNo

Analog InterfaceNoSynch Logical Channels1

Data Interface RS-232, V.24¥ V.120¥ Other: NoB CHANNEL PACKET

ISDN Interface S/TX.25 Term. SupportN/A

Power Interface PS1; PS2; External56/64 kbps112/128 kbpsNoNoAsync PAD

Self-Initializing?YesBonding?NoSync PAD

NIIGs: 2, 4, 6, 8, 20, 22, 25, 27Stores CallingNumber?TBA Logical Channels

NIPGs: 1-5, 7-8Dialing Modes: Auto Ans &Orig. Keypad; Dialing;Power On; MnemonicsAPIs Supported:

Additional Features:¥ Multiple CO configurations; including DMS and 5ESS Custom capability are part of the set software and called into use from the Man-Machine interface. No cartridges are required.¥ Field Upgradable from 286/V

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-122122

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1231234.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Telrad CommunicationsIDS - 286/D1VoiceOne Channel

135 Crossways Park DriveCircuit-DataOne Channel

Woodbury, NY 11797B Channel PacketNone

Erv Sloan(516) 921-8300D Channel PacketYes

NI-1 Date:NowPrice:Simultaneous activecallsTwo; one voice &one data (B or D)

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 24Async¥ V.120Yes - 38.4 KbpsX.25 Term. SupportNo

Speaker Phone? YesFeature Keys?Yes; 16¥ Other DMI - 19.2 KbpsT-link - 19.2 KbpsTelrad - 38.4 KbpsAsync PADSync PADYes; 9600No

Analog InterfaceNoSynch Logical Channels1

Data Interface RS-232, V.24¥ V.120¥ Other: NoB CHANNEL PACKET

ISDN Interface S/T¥ DMI - 56/64 Kbps¥ T-Link - 56/64 Kbps¥ Telrad - 56/64 KbpsX.25 Term. SupportN/A

Power Interface PS1; PS2; External56/64 kbps112/128 kbpsYesNoAsync PAD

Self-Initializing?YesBonding?NoSync PAD

NIIGs: 2-4, 6-8, 10, 11, 12, 15, 17, 21, 22, 25, 27Stores CallingNumber?TBA Logical Channels

NIPGs: 1-5, 7-8Dialing Modes: Auto Ans &Orig. Hayes AT; ExtendedHayes; Keypad; SpeedDialing; Power On;MnemonicsAPIs Supported:Hayes AT;Extended AT

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-124124Additional Features:¥ Multiple CO configurations; Rate adaption schemes and SYNC/ASYNC capability are part of the set software and called into use from the Man-Machine interface No cartridges are required.¥ D-channel messages and commands can be sent/received through the RS-232 data port. Useful for Call Management applications.¥ Field Upgradable from 286/V

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1251254.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Telrad CommunicationsIDS - 287/VVoiceOne Channel

135 Crossways Park DriveCircuit-DataNone

Woodbury, NY 11797B Channel PacketNone

Erv Sloan(516) 921-8300D Channel PacketNone

NI-1 Date:TBAPrice:Simultaneous activecallsOne Voice,

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?One

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 40Async¥ V.120 NoX.25 Term. SupportNo

Speaker Phone? Yes¥ OtherAsync PADNo

Feature Keys?Yes; 37Sync PADNo

Analog InterfaceNoSynch Logical Channels

Data Interface ¥ V.120¥ Other: NoB CHANNEL PACKET

ISDN Interface S/TX.25 Term. SupportN/A

Power Interface PS2; External56/64 kbps112/128 kbps No NoAsync PAD

Self-Initializing?YesBonding? NoSync PAD

NIIGs: 2, 4, 6Stores CallingNumber? Logical Channels

NIPGs: 1-5Dialing Modes: Keypad,Speed Dialing, Last No.Redial, Save & RepeatAPIs Supported:

Additional Features:¥ Multiple CO configurations; DMS Custom and 5ESS Custom are part of the Set software and called into use from the Man-Machine interface. No cartridges are required.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1261264.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Telrad CommunicationsIDS - 287/PVoiceOne Channel

135 Crossways Park DriveCircuit-DataOne Channel

Woodbury, NY 11797B Channel PacketNone

Erv Sloan(516) 921-8300D Channel PacketYes

NI-1 Date:TBAPrice:Simultaneous activecallsTwo, One Voice,One PMD

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 40Async¥ V.120NoX.25 Term. SupportNo

Speaker Phone? Yes¥ OtherAsync PADYes; 9600

Feature Keys?Yes; 37Sync PADNo

Analog InterfaceNoSynch Logical Channels1

Data Interface RS-232, V.24¥ V.120¥ Other: NoB CHANNEL PACKET

ISDN Interface S/T¥ Telrad - 56/64 KbpsX.25 Term. SupportN/A

Power Interface PS2; External56/64 kbps112/128 kbpsYesNoAsync PAD

Self-Initializing?YesBonding?NoSync PAD

NIIGs: 2, 4, 6, 8, 20, 22, 25, 27Stores CallingNumber? Logical Channels

NIPGs: 1-5, 7-8Dialing Modes:Auto Ans & Orig.; Keypad;Speed Dialing; Power On;Mnemonics; RedialAPIs Supported:

Additional Features:¥ Multiple CO configurations and DMS Custom and 5ESS Custom are part of the set software and called into use from the Man-Machine interface. No cartridges are required.¥ Field Upgradable from 287/V

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1271274.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Telrad CommunicationsIDS - 287/D1VoiceOne Channel

135 Crossways Park DriveCircuit-DataOne Channel

Woodbury, NY 11797B Channel PacketNone

Erv Sloan(516) 921-8300D Channel PacketYes

NI-1 Date:TBAPrice:Simultaneous activecallsTwo, One Voice,One CMD or PMD

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 40Async¥ V.120NoX.25 Term. SupportNo

Speaker Phone? Yes¥ OtherAsync PADYes; 9600

Feature Keys?Yes; 37Sync PADNo

Analog InterfaceNoSynch Logical Channels1

Data Interface RS-232, V.24¥ V.120¥ Other: NoB CHANNEL PACKET

ISDN Interface S/T¥ Telrad - 56/64 KbpsX.25 Term. SupportN/A

Power Interface PS2; External56/64 kbps112/128 kbpsYesNoAsync PAD

Self-Initializing?YesBonding?NoSync PAD

NIIGs: 2-4, 6-8, 10, 11, 12, 15, 17, 21, 22, 25, 27Stores CallingNumber? Logical Channels

NIPGs: 1-5, 7-8Dialing Modes:Auto Ans & Orig.; Keypad;Speed Dialing; Power On;MnemonicsAPIs Supported:

Additional Features:¥ Multiple CO configurations; DMS custom and 5ESS Custom are part of the set software and called into use from the Man-Machine interface. No cartridges are required.¥ Field Upgradable from 287/V

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1281284.2.4 ISDN PhonesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Telrad CommunicationsIDS - 287/D2VoiceOne Channel

135 Crossways Park DriveCircuit-DataOne Channel

Woodbury, NY 11797B Channel PacketNone

Erv Sloan(516) 921-8300D Channel PacketYes

NI-1 Date:TBAPrice:Simultaneous activecallsThree, One Voice,One CMD, OnePMD

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes, 2 x 40Async¥ V.120NoX.25 Term. SupportNo

Speaker Phone? Yes¥ OtherAsync PADYes; 9600

Feature Keys?Yes; 37Sync PADNo

Analog InterfaceNoSynch Logical Channels1

Data Interface RS-232, V.24¥ V.120¥ Other: NoB CHANNEL PACKET

ISDN Interface S/T¥ Telrad - 56/64 KbpsX.25 Term. SupportN/A

Power Interface PS2; External56/64 kbps112/128 kbpsYesNoAsync PAD

Self-Initializing?YesBonding?NoSync PAD

NIIGs: 2-4, 6-8, 10, 11, 12, 15, 17, 21, 22, 25, 27Stores CallingNumber? Logical Channels

NIPGs: 1-5, 7-8Dialing Modes:Auto Ans & Orig.; Keypad;Speed Dialing; Power On;Mnemonics; RedialAPIs Supported:

Additional Features:¥ Multiple CO configurations and SYNC/ASYNC capability are part of the set software and called into use from the Man-Machine interface No cartridges are required.¥ Field Upgradable from 287/V

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-129129