This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1191194.2.5 Single port ISDN LAN bridgesCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

Combinet, Inc.Everyware TM LCVoiceNone, future

333 West El Camino RealISDN BRI LAN BridgeCircuit-DataTwo Channels

Sunnyvale, CA 94087B Channel PacketNone

(408) 522 - 9020FAX: (408) 732 - 5479D Channel PacketNone

NI-1 Date:Currently SupportedPrice: $1690Simultaneous activecallsTwo, both data

NI-2 Date:2Q94FCC Class:A,B pendingUses 1 DN or 2?Either

Analog Interface:NoneCIRCUIT DATA56/64 kbpsYes Data Over Speech Bearer?No

Data Interface:Ethernet 10 Base-2112/128 kbps Yes Data Compression?No

Bonding? NoCalls on Demand?Yes

ISDN Interface:BRI: RJ-45Power120/220 VAC ExternalStores Calling Number orMAC address? YesAPIs Supported:Automatictransparent touser. Storednumber ondemand

Self-Initializing?YesDialing Modes:Automatic transparent touser. Stored number ondemandNIIGs:NIPGs:3,4,13,14,176

Additional Features:¥ Ethernet LAN Bridge to ISDN: Address learning, filter and forward: on demand 64 or 128¥ Configuration in nonvolatile memory.¥ Caller ID, password, Ethernet address ID accept/reject calls.¥ Call back of specified phone numbers¥ Supports remote configuration over Ethernet or ISDN, IP addressable¥ Compatible with Combinet Switched-56 products.Software/Operating Systems:MAC-layer bridge. Protocol, NOS, application transparent.Compatible with

ALL LAN software operating systems.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1201204.2.5 Single port ISDN LAN bridgesCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

Combinet, Inc.Everyware TM 150VoiceNone, future

333 West El Camino RealISDN BRI LAN Bridge(Single User)Circuit-DataTwo Channels

Sunnyvale, CA 94087B Channel PacketNone

(408) 522 - 9020FAX: (408) 732 - 5479D Channel PacketNone

NI-1 Date:Currently SupportedPrice: $990Simultaneous activecallsTwo, both data

NI-2 Date:2Q94FCC Class:A,B pendingUses 1 DN or 2?Either

Analog Interface:NoneCIRCUIT DATA56/64 kbpsYes Data Over Speech Bearer?No

Data Interface:Ethernet 10 Base-T112/128 kbps Yes Data Compression?Yes

Bonding? NoCalls on Demand?Yes

ISDN Interface:BRI: RJ-45Power120 VAC ExternalStores Calling Number orMAC address? YesAPIs Supported:Automatictransparent touser. Storednumber ondemand

Self-Initializing?YesDialing Modes:Automatic transparent touser. Stored number ondemandNIIGs:NIPGs:3,4,13,14,176

Additional Features:¥ Ethernet LAN Bridge to ISDN: Address learning, filter and forward: on demand 64 or 128¥ Configuration in nonvolatile memory.¥ Caller ID, password, Ethernet address ID accept/reject calls.¥ Call back of specified phone numbers¥ Supports remote configuration over Ethernet or ISDN, IP addressable¥ Compatible with Combinet Switched-56 products.Software/Operating Systems:MAC-layer bridge. Protocol, NOS, application transparent.Compatible with

ALL LAN software operating systems.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1211214.2.5 Single port ISDN LAN bridgesCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

Combinet, Inc.Everyware TM 200VoiceNone, future

333 West El Camino RealISDN BRI LAN BridgeCircuit-DataTwo Channels

Sunnyvale, CA 94087B Channel PacketNone

(408) 522 - 9020FAX: (408) 732 - 5479D Channel PacketNone

NI-1 Date:Currently SupportedPrice: $2190Simultaneous activecallsTwo, both data

NI-2 Date:2Q94FCC Class:A,B pendingUses 1 DN or 2?Either

Analog Interface:NoneCIRCUIT DATA56/64 kbpsYes Data Over Speech Bearer?No

Data Interface:Ethernet:10 Base-T10 Base-2112/128 kbps Yes Data Compression?Yes

Bonding? NoCalls on Demand?Yes

ISDN Interface:BRI: RJ-45Power 120/220VAC ExternalStores Calling Number orMAC address? YesAPIs Supported:Automatictransparent touser. Storednumber ondemand

Self-Initializing?YesDialing Modes:Automatic transparent touser. Stored number ondemandNIIGs:NIPGs:3,4,13,14,176

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-122122Additional Features:¥ Ethernet LAN Bridge to ISDN: Address learning, filter and forward: on demand 64 or 128¥ Configuration in nonvolatile memory.¥ Caller ID, password, Ethernet address ID accept/reject calls.¥ Call back of specified phone numbers¥ Supports remote configuration over Ethernet or ISDN, IP addressable¥ Compatible with Combinet Switched-56 products.Software/Operating Systems:MAC-layer bridge. Protocol, NOS, application transparent.Compatible with

ALL LAN software operating systems.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1231234.2.5 Single port ISDN LAN bridgesCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

Combinet, Inc.Everyware TM 400VoiceNone, future

333 West El Camino RealISDN BRI LAN BridgeCircuit-DataTwo Channels

Sunnyvale, CA 94087B Channel PacketNone

(408) 522 - 9020FAX: (408) 732 - 5479D Channel PacketNone

NI-1 Date:Currently SupportedPrice: $2190Simultaneous activecallsTwo, both data

NI-2 Date:2Q94FCC Class:A,B pendingUses 1 DN or 2?Either

Analog Interface:NoneCIRCUIT DATA56/64 kbpsYes Data Over Speech Bearer?No

Data Interface:Ethernet:10 Base-T10 Base-2112/128 kbps Yes Data Compression?Yes

Bonding? NoCalls on Demand?Yes

ISDN Interface:BRI: RJ-45Power 120 VAC InternalStores Calling Number orMAC address? YesAPIs Supported:Automatictransparent touser. Storednumber ondemand

Self-Initializing?YesDialing Modes:Automatic, transparent touser. Stored number ondemandNIIGs:NIPGs:3,4,13,14,176

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-124124Additional Features:¥ Ethernet LAN Bridge to ISDN: Address learning, filter and forward: on demand 64 or 128¥ Configuration in nonvolatile memory.¥ Caller ID, password, Ethernet address ID accept/reject calls.¥ Call back of specified phone numbers¥ Supports remote configuration over Ethernet or ISDN, IP addressable¥ Compatible with Combinet Switched-56 products.Software/Operating Systems:MAC-layer bridge. Protocol, NOS, application transparent.Compatible with

ALL LAN software operating systems.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1251254.2.5 Single port ISDN LAN bridgesCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

Develcon Electronics LimitedI-Gate Model 150VoiceNot Applicable

856 51st Street EastSaskatoon, SK CanadaEthernet MAC Layerlearning bridge withCircuit-DataTwo Channels

S7K 5C7Erich Kirchnerintegral ISDNB Channel PacketNo

(306) 933 - 3300FAX (306) 931 - 1370D Channel PacketNo

NI-1 Date:NowPrice: $2695 (US)Simultaneous activecallsTwo

NI-2 Date:TBAFCC Class:AUses 1 DN or 2?Either

Analog Interface:CIRCUIT DATA56/65 kbpsYes Data Over Speech Bearer?No

Data Interface:Ethernet10 Base 5 or10 Base 2112/128 kbpsYes Data Compression?To be released(Call foravailability)

ISDN Interface:S/T (RJ-45)Bonding?Calls on Demand?Yes

PowerExternalStores Calling Number orMAC address?YesAPIs Supported:N/A

Self-Initializing?YesDialing Modes:NIIGs:NIPGs:3, 14

Additional Features:LAN protocol independentOperates with AT&T, Northern Telelcom, and National ISDN-1. Also certified to ETSI (Net 3),Japan (INSNet 64), New ZealandTime-of -day connection facility.Bandwidth on demand support.Advanced filtering capabilities. (Programmable over complete Ethernet Frame)Auto connect based on LAN data.SNMP support.Software/Operating Systems:N/A - Protocol transparent

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1261264.2.5 Single port ISDN LAN bridgesCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

DigiBoardIMACVoiceTwo Channels

6400 Flying Cloud DriveCircuit-DataTwo Channels

Eden Prairie, MN 55344B Channel Packet

Jim Libersky1-800-344-4273D Channel Packet

NI-1 Date:NowPrice: $ 1,695Simultaneous activecallsTwo

NI-2 Date:1994FCC Class:BUses 1 DN or 2?Either

Analog Interface: N/ACIRCUIT DATA56/65 kbps Yes Data Over Speech Bearer?Yes

Data Interface: Ethernet 10B2, 10B5112/128 kbpsYes Data Compression?IndustryStandard

Bonding? Notat presentCalls on Demand?Yes

ISDN Interface: RJ-45Stores Calling Number orMAC address? YesAPIs Supported:

Power ExternalNIIGs:

Self-Initializing?Dialing Modes: Manual and AutoNIPGs:

Additional Features:¥ Multipoint or Point to Point¥ Switched Voice or Switched Data¥ D-channel protocol analyzer¥ SNMP managementSoftware/Operating Systems:¥ Supports IPX/SPX, TCP/IP, NETBIOS, Appletalk, and all other Ethernet protocols

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1271274.2.5 Single port ISDN LAN bridgesCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

Gandalf Systems Corp.LANLINE 5240VoiceNo

Cherry Hill Industrial Ctr.Building 9Circuit-DataTwo

Cherry Hill, NJ 08003B Channel PacketNo

609-424-9400D Channel PacketNo

NI-1 Date: NowPrice: 2495Simultaneous activecalls2

NI-2 Date:FCC Class: AUses 1 DN or 2?Either

Analog Interface:CIRCUIT DATA56/65 kbps Yes Data Over Speech Bearer?Optional

Data Interface: Ethernet: AUI, BNC112/128 kbpsYes Data Compression?Yes, 8:1

Bonding? NoCalls on Demand?Yes

ISDN Interface: S/T or UStores Calling Number orMAC address?APIs Supported:

Power ExternalNIIGs:3,14

Self-Initializing? YesDialing Modes: AutomaticNIPGs:6

Additional Features:¥ Time of Day programmable¥ PPP link protocol with chap security¥ Optional integral NT-1¥ Optional support for dedicated WAN link in addition to ISDNSoftware/Operating Systems:¥ Routing option for TCP/IP and IPX (Novell)¥ SNMP management¥ Remote configuration & management

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1281284.2.5 Single port ISDN LAN bridgesCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

Gandalf Systems Corp.LANLINE 5510VoiceOne

Cherry Hill Industrial Ctr.Building 9Circuit-DataOne

Cherry Hill, NJ 08003B Channel PacketNo

609-424-9400D Channel PacketNo

NI-1 Date:NowPrice: 1495Simultaneous activecallsTwo

NI-2 Date:FCC Class:Uses 1 DN or 2?Either

Analog Interface:RJ-11CIRCUIT DATA56/65 kbps Yes Data Over Speech Bearer?Optional

Data Interface:EthernetUTP, AVI, BNC112/128 kbpsNo Data Compression?No

Bonding? NoCalls on Demand?Yes

ISDN Interface:S/TStores Calling Number orMAC address? YesAPIs Supported:

PowerExternalNIIGs:2,3,4,11

Self-Initializing?YesDialing Modes: Hayes AT,front panel & automaticNIPGs:1, 6

Additional Features:¥ Concurrent LAN bridging and voice supportSoftware/Operating Systems:¥ Transparent to LAN protocols

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1291294.2.5 Single port ISDN LAN bridgesCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

ISCOM, Inc.Translan,VoiceNo

6103 Baltimore Avenue, 205Riverdale, MD 20737LAN to LANCircuit-Data2 Channels interconnectionB Channel Packet2 Channels

Phone/FAX: (301) 779 - 1368D Channel PacketNo

NI-1 Date:NowPrice:Simultaneous activecalls1

NI-2 Date:1994FCC Class:Uses 1 DN or 2?1

Analog Interface:NoCIRCUIT DATA56/65 kbpsYes Data Over Speech Bearer?No

Data Interface:ISA Bus112/128 kbpsNo Data Compression?No

Bonding?NoCalls on Demand?Yes

ISDN Interface:S/TStores Calling Number orMAC address?YesAPIs Supported:Hayes AT

PowerISA BusNIIGs:3, 5, 14, 16, 19

Self-Initializing?NoDialing Modes:NIPGs:6, 9, 10

Additional Features:¥ You will be able to choose between: Router to Router or Remote to Router based on software choices¥ International callsSoftware/Operating Systems:¥ DOS, UNIX, Novell, TCP/IP