This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1634.2.8 PRI AdaptersCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

DGM&S Inc.Multi-Protocol AdapterFull featured ISA or VMS Bus Platform

1025 Briggs RoadMt. Laurel, NJ 08054DSP (MPAD)for support of ISDN PRI and SS7 interfaceapplications.

(609) 866 - 1212

NI-1 Date:NowNI-2 Date:12/93Price:$2,395(Single Quantities)PortsFull T1 - Handles up to sixB channels; additionalB channels can be added

Voice Interfaces:Through T1Data Interfaces:V.35, T1Split and combine Bchannels?B channel can beswitched toON-Board orOFF-Boarddestinations

Bonding?Not available butcan be supportedon-board

ISDN Interface:T1

Power:From Host

PC/Workstation

Additional Features:The MPAD is a multi-purpose platform that can be used for variety of ISDN or SS7 applications. It isintended to be utilized as a development platform for prototype or target platform development. Thehigh powered Texas Instruments C30 Digital Signal Processor provides power for data manipulationincluding inverse multiplexing, compression or other multimedia features and functions.Software/Operating Systems:Runs under DGM&S QRux Operating System (Provided with DGM&S QSource PRI Software) or withany typical embedded OS including pSOS and VRTX.QSource (TM) is a trademark of DGM&S, Inc.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1644.2.8 PRI AdaptersCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Gandalf Systems Corp.Access SDXPRI channel bank

Cherry Hill Industrial Ctr.and gateway for data applications

Building 9Cherry Hill, NJ 08003

609-424-9400

NI-1 Date:NowNI-2 Date:June 94Price:Base Unit withone PRI $12,000PortsUp to 6, PRI

Voice Interfaces:Data Interfaces:Split and combine Bchannels? Yes, up to 30

R5-232V.35Bonding? No, prop.

V.11 ISDN Interface: PRI, ESF-DS1

RS-422/3EthernetPower:External

Additional Features:¥ Dial on control lead, permanent calls, & interactive call setup¥ N x 64 Kbps support to 1920 Kbps¥ Telnet configuration and call control using LAN interface¥ B channel packet supportSoftware/Operating Systems:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1654.2.8 PRI AdaptersCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

ISCOM, Inc.6103 Baltimore Avenue, 205Datavoice S2 PC CardISDN S2 card (Primary rate 30 B+D or 23B+D for T1 network) offering B and D

Riverdale, MD 20737channels management at n x 64 Kbps.

Phone/FAX: (301) 779 - 1368

NI-1 Date:NowNI-2 Date:1994Price:PortsT1, S2

Voice Interfaces:Data Interfaces:Split and combine Bchannels?n x 64, 23B+D

NoneISA BusBonding?No

ISDN Interface:S/T

Power:Bus

Additional Features:Supports 6, 9, 10 NIPGsSoftware/Operating Systems:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1664.2.8 PRI AdaptersCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Mitel CorporationEnhanced Dual48 channel (T1) or 60 channel (E1) Primary

Communicating ObjectsP.O. Box 13089T1/E1 CardRate PC Plug in Card. Has on-boardprocessor for signalling. MVIP compatible.

360 Legget DriveKanata, Ontario, Canada(MB89112/122)Facility Data Line handled via HDLCDevices.

K2K 1X3(613) 592-2122FAX: (613) 592-4784

NI-1 Date:NI-2 Date:Price:Ports 2 T1 or 2 E1 ports 48/60 channels

Voice Interfaces:Data Interfaces:Split and combine Bchannels?

Analog Handler InterfaceHDLC devices for packedmode data PC Bus andMVIP Bus for circuitswitched dataBonding?

ISDN Interface:T1 or E1

Power: From PC

Additional Features:Combines either the 71 1.544 17 bps interfaces or two 2.048 Mbps interfaces (MB89122) or aPC compatible plug in card. An on-board processor handles ISDN layer two and three signallingprotocols. The card includes a 512 channel Enhanced Compliant MVIP switch matrix to providetime switching within the card as well as for the 256 channel MVIP Bus.Software/Operating Systems:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1674.2.8 PRI AdaptersCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Mitel CorporationSingle T1/E1 Card24 channel (T1) or 30 channel (E1) Primary

Communicating ObjectsP.O. Box 13089(MB89111/121)Rate PC plug-in card for bridges, routers,X.25 gateways, inverse Muxes, Mux/

360 Legget DriveKanata, Ontario, CanadaDMuxes, Communications controllers

K2K 1X3(613) 592-2122FAX: (613) 592-4784

NI-1 Date:NI-2 Date:Price:Ports1 T1 or 1 E1 port 24/48 channels

Voice Interfaces:Data Interfaces:Split and combine Bchannels?

Analog Handset Interface HDLC Resources PC Bus MVIP BusBonding?

ISDN Interface:T1 or E1

Power: From PC

Additional Features:The MB provides a Primary Rate Compatible communications interface for PC-based equipmentcontaining either a T1 1.544 Mbps interface (MB89111) or an E1 2.048 Mbps Interface (MB89121).An on-board 9LL ensures compliance to assume 1.5 specifications. The card contains a digitalswitching matrix for connection to an MVIP Bus and for local switching.Software/Operating Systems:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1684.2.8 PRI AdaptersCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Mitel Corporation Dual T1/E1 Card48 channel (T1) or 60 channel (E1)

Communicating ObjectsP.O. Box 13089(MB89110/120)Primary interface. Applications bridge,router, X.25 gateways, inverse Mux,Mux/DMux, Communication controller

360 Legget DriveKanata, Ontario, Canada

K2K 1X3(613) 592-2122FAX: (613) 592-4784

NI-1 Date:NI-2 Date:Price:Ports 2 T1 or 2 E1 Ports 48/60 Channels

Voice Interfaces:Data Interfaces:Split and combine Bchannels?

Four HDLCResourcesBonding?

PC BusMVIP BusISDN Interface:T1 or E1

Power: From PC

Additional Features:The MB89110/120 provides a Primary Rate-compatible communications interface for PC-basedequipment containing either two T1 1.544 Mbps interfaces (MB89110) or two E1 2.042 Mbpsinterfaces (MB89120).There is also an analog handset interface to record messages or monitor traffic.Four HDLC resources provide common channel/Facility Data Link (FDL) signalling support.Digital PLI provides timing generation.The card includes a 512 channel Enhanced Compliant MVIP switch matrix to provide time switchingwithin the card as well as for the 256 channel MVIP bus. This allows the MB89110/120 to act as acentral communications/switching resource in an MVIP system.Software/Operating Systems:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1694.2.8 PRI AdaptersCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Nitech, Inc.NiteOwl 2230Primary rate 30B+D or 23B+D,

(New Information Technologies,Inc.)PC BasedAdapter Cardoffering B and D Channel managementat n x 64 kbps

4400 Route 9 SouthFreehold, NJ 07728

Dilip Guha(908) 303-7471

NI-1 Date:NowNI-2 Date:1994Price:PortsUp to 8 PRIs

Voice Interfaces:YesData Interfaces:Split and combine Bchannels? Yes

T1, V.35, RS-232, RS-449Bonding? No

ISDN Interface: T1

Power: From PC

Additional Features:¥ The 2230 NiteOwl is a PC-based PRI Adapter which can also monitor and simulate PRI, LAPD/X,25. Q.921/Q.920 at the T-1 interface¥ It supports fractional T-1 up to 2.048 Mbps and can simulate all 24 or 32 channels simultaneously.¥ B channel packet supportSoftware/Operating Systems:¥ Microsoft Windows

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1704.2.8 PRI AdaptersCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Primary Rate IncorporatedPRI-48TM DualT1/ISDN Communications Controller

5 Manor ParkwaySalem, NH 03079T1/ISDN VMEControllerwith non-blocking DS0 Switching matrix

(603) 898 - 1800

Sales 1- 800- 950 - ISDN (4736)

NI-1 Date:N/ANI-2 Date:07/01/93Price:$6250Ports:¥ Two T1 Interfaces

Voice Interfaces: 23 ChannelsData Interfaces:Split and combine Bchannels?Yes

¥VME Bus¥TDM HighwayBonding?YesMode 0,1

¥Optional DS1, V.35,RS.449, DSX.1ISDN Interface:S/T or U (dual)

Power:From Bus

Additional Features:¥ Direct access to T1, fractional T1, and Primary Rate¥ VME slave interface to host¥ Supports 24 full duplex HDLC data streams¥ D and B channel packet¥ V.120 Multiplexing onto channels from 64 Kbps to 1.5 Mbps¥ Suited for frame relay and call relay circuits¥ Also supports SW56 robbed-bit dialing modes and on-Board DS0 switching. Non-Facility associated signaling (NFAS)Software/Operating Systems:¥ Complete ISDN Software¥ UNIX, VRTX, VXWorks, OS9, VME Exec, POS¥ PRI�s SMI Programming Interface

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1714.2.8 PRI AdaptersCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Primary Rate IncorporatedPRI-ISA48TM DualT1/ISDN Communications Controller

5 Manor ParkwaySalem, NH 03079T1/ISDN Controller

(603) 898 - 1800

Sales 1- 800- 950 - ISDN (4736)

NI-1 Date:N/ANI-2 Date:07/01/93Price:$3950Ports:¥ Two T1 Interfaces

Voice Interfaces: 23 ChannelsData Interfaces:Split and combine Bchannels?Yes

¥ISA Bus¥Optional DS1, V.35,Bonding?YesMode 0,1

RS.449, DSX.1¥TDM Highway ISDN Interface:S/T or U (dual)

Power:From Bus

Additional Features:¥ Direct access to T1, fractional T1, and Primary Rate¥ ISA slave interface to host¥ Supports 24 full duplex HDLC data streams¥ D and B channel packet¥ V.120 Multiplexing onto channels from 64 Kbps to 1.5 Mbps¥ Suited for frame relay and call relay circuits¥ Also supports SW56 robbed-bit dialing modes and on-Board DS0 switching.¥ Non-facility associated signaling (NFAS)Software/Operating Systems:¥ Complete ISDN Software¥ SCO Unix, OS2, DOS¥ PRI�s SMI Programming Interface