This information is subject to change without notice.See Notice of Disclaimer on Title Page.3-13.National ISDN SolutionsThis section consists of three parts, each containing application guides highlightingthe features of a specific ISDN interface. Section 3.1 contains guides which useNational ISDN-1 Basic Rate Interfaces (BRIs). Section 3.2 contains guides toillustrate the additional functionality of the National ISDN-2 BRI. Although theyare not repeated here for space reasons, all the guides in Section 3.1 could also beimplemented using NI-2 BRI. Section 3.3 demonstrates solutions using theNational ISDN-2 Primary Rate Interface (PRI).Each guide in the Catalog contains the following components (in order ofpresentation): an application description with potential benefits to the end user, theconfiguration of the example solution identifying alternate configurations, a shortdescription of how the solution works, equipment required, and capabilities to berequested from the ISDN service provider. Each guide concludes with "technicalnotes" which provide further details about the operation of the solution and possibleoptions. Additional implementation information, which is of particular interest toequipment designers, application developers and system integrators, is provided inSection 5 of this Catalog. This supplementary material is referenced where usefulin the Technical Notes.Integrated Voice and Data Terminal Configurations for BRI SolutionsIn many applications, the users benefit from integrated voice and data. Theirphones and computers are closely coupled in an "integrated voice and data system",and both take advantage of ISDN.With the variety of products available, the users can "package" their phone,personal computers and connection to ISDN in one of several ways. To demonstratethis flexibility, yet not exhaust the overwhelming number of possibilities, thisdocument focuses on five typical packages. Most of the BRI guides in Sections 3.1and 3.2 utilize one of the five packages, or configurations, shown below. BecausePRI configurations are more complex, no similar packaging for PRI is used in theguides in Section 3.3.The guides in the catalog are example solutions. Above most of the solution guides’configuration diagram, a list of configuration numbers appears. Because of spacelimitations, only the configuration number in bold and underlined (e.g.,

2) is fullyexplained in the guide. The other configuration numbers shown identify packagingalternatives for that solution, but other alternatives may exist.

This information is subject to change without noticeSee Notice of Disclaimer on Title Page3-21.Personal Computer (or workstation)equipped with an ISDN Adapter

This information is subject to change without notice.See Notice of Disclaimer on Title Page.3-32.ISDN Phone with Personal ComputerinterfaceISDNPhone

This information is subject to change without noticeSee Notice of Disclaimer on Title Page3-43.ISDN Terminal Adapter with PersonalComputer and phone interface

NT-1

TerminalAdapterConfiguration 3PersonalComputer

ISDNPhone

This information is subject to change without noticeSee Notice of Disclaimer on Title Page3-65.Personal Computer (or workstation) withLAN interface and ISDN LAN BridgeAnalog Phone