This information is subject to change without notice.See Notice of Disclaimer on Title Page4-86864.2.3 Attendant ConsolesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Tone Commander Systems1030DVoice2 Channels

4370 150th Ave. NE10 line/30 stationISDN Attendant ConsoleCircuit-DataNone

Redmond, WA 98073(ATT #5 ESSCompatible)B Channel PacketNone

Norton Lovold(800) 524-0024D Channel PacketNone

NI-1 Date:Price: $2,885.00Simultaneous activecalls2

NI-2 Date:FCC Class:AUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes (1x20)Async¥ V.120NoX.25 Term. SupportNo

Speaker Phone? No¥ OtherAsync PADNo

Feature Keys? Yes (11)Sync PADNo

Analog Interface Yes RJ21XSynch Logical Channelsn/a

Data Interface n/a¥ V.120¥ OtherNoB CHANNEL PACKET

ISDN Interface S/TX.25 Term. SupportNo

Power Interface External56/64 kbpsn/aAsync PADNo

Self-Initializing? Yes112/128 kbpsn/aSync PADNo

NIIGs: 2,10Bonding?No Logical Channelsn/a

Stores Calling Number? YesAPIs Supported:n/a

NIPGs: 1,2,4,5DialingModes: Keypad andRepertory Dialing

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-8787Additional Features:Full Analog and Digital Attendant Console features:- 10 Attendant lines/30 station DSS/BLF- Mix of analog and digital station monitoring- Auto Call Splitting- Inbound Call Queue- Programmable Calling Name/Calling Line Display- Camp-On/Timed Hold reminder- Programmable Ring Delays

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-88884.2.3 Attendant ConsolesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Tone Commander Systems1560DVoice2 Channels

4370 150th Ave. NE15 line/60 station ISDNAttendant ConsoleCircuit-DataNone

Redmond, WA 98073(ATT #5 ES Compatible)B Channel PacketNone

Norton Lovold(800) 524-0024D Channel PacketNone

NI-1 Date:Price: $4,435.00Simultaneous activecalls2

NI-2 Date:FCC Class:AUses 1 DN or 2?Either

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes (1x20)Async¥ V.120NoX.25 Term. SupportNo

Speaker Phone? No¥ OtherAsync PADNo

Feature Keys? Yes (11)Sync PADNo

Analog Interface Yes RJ21XSynch Logical Channelsn/a

Data Interface n/a¥ V.120¥ OtherNoB CHANNEL PACKET

ISDN Interface S/TX.25 Term. SupportNo

Power Interface External56/64 kbpsn/aAsync PADNo

Self-Initializing? Yes112/128 kbpsn/aSync PADNo

NIIGs: 2,10Bonding?n/a Logical Channelsn/a

NIPGs: 1,2,4,5Stores Calling Number? YesAPIs Supported:n/a

DialingModes:Keypad andRepertory Dialing

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-8989Additional Features:Full Analog and Digital Attendant Console features:- 15 Attendant lines/60 station DSS/BLF- Mix of analog and digital station monitoring- Auto Call Splitting- Inbound Call Queue- Programmable Calling Name/Calling Line Display- Camp-On/Timed Hold reminder- Programmable Ring Delays

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-90904.2.3 Attendant ConsolesCOMPANY NAMEPRODUCT NAME CALLS SUPPORTED

Tone Commander Systems40D/120Voice1 Channel

4370 150th Ave. NERedmond, WA 98073Expandable ISDNAttendant Console withCircuit-DataNone

240 station DSS/BLFB Channel PacketNone

Norton Lovold(800) 524-0024D Channel PacketNone

NI-1 Date:1Q94Price: $2,500-Console$1,500-120 station DSSSimultaneous activecalls1

NI-2 Date:1Q94FCC Class:AUses 1 DN or 2?1

VOICE AND DISPLAYCIRCUIT DATAD CHANNEL PACKET

Display Yes (4x40)Async¥ V.120NoX.25 Term. SupportNo

Speaker Phone? No¥ OtherAsync PADNo

Feature Keys? YesSync PADNo

Analog Interface NoSynch Logical Channelsn/a

Data Interface n/a¥ V.120¥ OtherNoB CHANNEL PACKET

ISDN Interface UX.25 Term. SupportNo

Power Interface External56/64 kbpsn/aAsync PADNo

Self-Initializing? Yes112/128 kbpsn/aSync PADNo

NIIGs: 10Bonding?No Logical Channelsn/a

NIPGs: 1,2,4,5Stores Calling Number? YesAPIs Supported:n/a

DialingModes:Keypad andRepertory Dialing

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-9191Additional Features:Advanced Attendant Call Processing features:- Expandable to 240 station DSS/BLF- Switched Loop Call Processing- Prioritized Inbound Call Queue- Programmable Calling/Called Party Name Displays- Camp-On/Call Park/Timed Hold reminder- Auto Call Splitting - Screened/Unscreened Call Transferring- Multi-Party Conference- Network Diagnostic Displays