This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1281284.2.6 Communications servers, routers, bridges, multiport ISDN LANBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Advanced ComputerCommunicationsNileStandalone, Multiprotocol,Remote Bridge/Router for TCP/IP, IPX,

10261 Bubb RoadXNS, DecNet, AppleTalk

Cupertino, CA 95014

(408) 864-0600FAX: (408) 446-5234

NI-1 Date:Not announcedNI-2 Date:Not announcedPrice:$3,750 - $5,050Ports 3

Voice Interfaces:NoneData Interfaces:BRI-ISDN4/16 Mb Token Ring10 Base 210 Base 510 Base TV.35RS-422/449X-21RS-232Split and combine Bchannels?Bonding?YesNo

ISDN Interface:S/T

Power:110/220 vac

Additional Features:¥ Field replaceable LAN and WAN interfaces¥ 1 or 2 WAN portsSoftware/Operating Systems:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1291294.2.6 Communications servers, routers, bridges, multiport LAN ISDNBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Ascend Communications, Inc.Pipeline Access Routers¥ LAN-to-LAN routing

1275 Harbor Bay Parkway¥ Telecommuting with Client-to-LAN

Alameda, CA 94501 routing

(510) 769-6001¥ Remote access to corporate LAN

NI-1 Date:11/92NI-2 Date:10/93Price: Start at $3.3KPortsT1/E1, 4 BRI/4 SW56 (2w & 4w)1 BRI/SW56

Voice Interfaces:T1 Drop & InsertPRI to T1 conversionData Interfaces: RS-232Split and combine Bchannels? Bonding? ISDN Interface:YesPacket InverseMultiplexingS/T

Power: 90-130 VAC, 0.7-1.4 A, 220-240 VAC, 0.34-0.7 A, 47-63 Hz

Additional Features:Five levels of security; integrated digital modems to support analog dial-in modems; optional Ethernet10 BaseT hub; optional serial ports; SNMP, remote access, CDR, WAN loopback, usage cappingSoftware/Operating Systems:Flash memory, Field upgradable

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1301304.2.6 Communications servers, routers, bridges, multiport LAN ISDNBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Ascend Communications, Inc.Pipeline MAXBandwidth manager for data networking,

1275 Harbor Bay ParkwayPBX integration and videoconferencing;dial in WAN hub for telecommuting

Alameda, CA 94501and remote access to Corp-LAN

(510) 769-6001

NI-1 Date:N/ANI-2 Date:10/93Price: starts at $10KPortsT1/E1, up to 4 PRI

Voice Interfaces:T1 Drop & InsertPRI to T1 conversionData Interfaces: RS-449 V.35 X.21Split and combine Bchannels? Bonding? ISDN Interface:YesPacket InverseMultiplexingPRI

Power: 90-130 VAC, 0.7-1.4 A, 220-240 VAC, 0.34-0.7 A, 47-63 Hz

Additional Features:¥ LAN-to-LAN routing for TCP/IP¥ Remote access routing functionality¥ Call management - CDR (Call Detail Recording)¥ Network Management - such as SNMP + WAN loopback¥ Optional digital modems to support analog dial-in modemsSoftware/Operating Systems:Flash memory, field upgradable

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1311314.2.6 Communications servers, routers, bridges, multiport ISDN LANBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Cisco Systems Inc.1525 O�Brien DriveMenlo Park, CA 94025Cisco 2500Models 2503 Multi-Protocol router

Contact: Cisco Systems Inc.Certified for use in Europe, Japan, NorthAmerica, Australia

415-326-1981415-326-1989 (fax)

NI-1 Date: 1993NI-2 Date: N/APrice:$3195Ports2 x serial,1 BRI and Ethernet

Voice Interfaces: N/AData Interfaces:BRI, serial(V.35, RS-232, RS-449),EthernetSplit and combine Bchannels?Bonding?Split onlyNo

ISDN Interface:BRI

Power: 110/220 VAC

Additional Features:¥Support for multiple protocols, bridging, Dial on Demand Routing, Frame Relay, SMDS, X.25, DataCompression and Auto Install capability.Software/Operating Systems:¥Proprietary

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1321324.2.6 Communications servers, routers, bridges, multiport ISDN LANBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Cisco Systems Inc.1525 O�Brien DriveMenlo Park, CA 94025Cisco 2500Models 2504 Multi-Protocol router

Contact: Cisco Systems Inc.Certified for use in Europe, Japan, NorthAmerica, Australia

415-326-1981415-326-1989 (fax)

NI-1 Date: 1993NI-2 Date: N/APrice:$ 5,195Ports2 x serial,1 BRI and Token Ring

Voice Interfaces: N/AData Interfaces:BRI, serial(V.35, RS-232, RS-449),Token RingSplit and combine Bchannels?Bonding?Split onlyNo

ISDN Interface:BRI

Power: 110/220 VAC

Additional Features:¥Support for multiple protocols, bridging, Dial on Demand Routing, Frame Relay, SMDS, X.25, DataCompression and Auto Install capability.Software/Operating Systems:¥Proprietary

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1331334.2.6 Communications servers, routers, bridges, multiport ISDN LANBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Cisco Systems Inc.1525 O�Brien DriveMenlo Park, CA 94025Cisco 3000Models 3103 Multi-Protocol router

Contact: Cisco Systems Inc.Certified for use in Europe, Japan, NorthAmerica, Australia

415-326-1981415-326-1989 (fax)

NI-1 Date: 1993NI-2 Date: N/APrice:$ 5,295Ports1 BRI and Ethernet

Voice Interfaces: N/AData Interfaces:BRI, serial(V.35, RS-232, RS-449),EthernetSplit and combine Bchannels?Bonding?Split onlyNo

ISDN Interface:BRI

Power: 110/220 VAC

Additional Features:¥Support for multiple protocols, bridging, Dial on Demand Routing, Frame Relay, SMDS, X.25, DataCompression and Auto Install capability.Software/Operating Systems:¥Proprietary

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1341344.2.6 Communications servers, routers, bridges, multiport ISDN LANBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Cisco Systems Inc.1525 O�Brien DriveMenlo Park, CA 94025Cisco 3000Models 3104 Multi-Protocol router

Contact: Cisco Systems Inc.Certified for use in Europe, Japan, NorthAmerica, Australia

415-326-1981415-326-1989 (fax)

NI-1 Date: 1993NI-2 Date: N/APrice:$ 5,795Ports2 x serial,1 BRI and Ethernet

Voice Interfaces: N/AData Interfaces:BRI, serial(V.35, RS-232, RS-449),EthernetSplit and combine Bchannels?Bonding?Split onlyNo

ISDN Interface:BRI

Power: 110/220 VAC

Additional Features:¥Support for multiple protocols, bridging, Dial on Demand Routing, Frame Relay, SMDS, X.25, DataCompression and Auto Install capability.Software/Operating Systems:¥Proprietary

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1351354.2.6 Communications servers, routers, bridges, multiport ISDN LANBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Cisco Systems Inc.1525 O�Brien DriveMenlo Park, CA 94025Cisco 3000Models 3204 Multi-Protocol router

Contact: Cisco Systems Inc.Certified for use in Europe, Japan, NorthAmerica, Australia

415-326-1981415-326-1989 (fax)

NI-1 Date: 1993NI-2 Date: N/APrice:$ 6,995Ports2 x serial,1 BRI andToken Ring

Voice Interfaces: N/AData Interfaces:BRI, serial(V.35, RS-232, RS-449),Token RingSplit and combine Bchannels?Bonding?Split onlyNo

ISDN Interface:BRI

Power: 110/220 VAC

Additional Features:¥Support for multiple protocols, bridging, Dial on Demand Routing, Frame Relay, SMDS, X.25, DataCompression and Auto Install capability.Software/Operating Systems:¥Proprietary

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1361364.2.6 Communications servers, routers, bridges, multiport ISDN LANBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Connective Strategies, Inc.(CSI)PRI-MPG“LAN Router for remote user access

4500 Southgate Place, Ste. 100Primary Rate InterfaceMulti-Protocol Gateway

Chantilly, VA 22021

(703) 802-0023

NI-1 Date:NI-2 Date:1Q’94Price: $30,985Ports1 to 4 PRIs

Voice Interfaces:NoneData Interfaces: Ethernet 10 Base 2 10 Base 5 Token RingSplit and combine Bchannels?Bonding?YesNo

ISDN Interface:1 to 4 PRI

Power: External

Additional Features:¥ Hardware includes integrated floppy and hard disks, a 320 Mbps VME bus, one PRI port and one Ethernet or Token Ring port.¥ A total of four PRI ports and two Ethernets or one Token Ring port can be supported.Software/Operating Systems:¥ IP router option allows remote users to access TCP/IP LANS - Novell, LAN Manager, NFS - at speeds up to 128 KbpsPRI-MPG is a trademark of CSI

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1371374.2.6 Communications servers, routers, bridges, multiport LAN ISDNBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

DigiBoardDUAL IMACMAC Layer Ethernet Bridge

6400 Flying Cloud DriveProvides two connections to support four

Eden Prairie, MN 55344simultaneous calls, or provide a single 256kbps channel

Jim Libersky1-800-344-4273

NI-1 Date:NowNI-2 Date:1994Price: $2795Ports2

Voice Interfaces:Data Interfaces:AUI Port - Ethernet10B2, 10B5Split and combine Bchannels? Bonding? ISDN Interface:YesNoS/T (RJ-45)

Power: External

Additional Features:¥ SNMP MIB II¥ Transparent Connection Management¥ Remote Control Operation over Ethernet or ISDN¥ Ethernet & ISDN protocol analyzer built in¥ Compatible with any CCITT Certified Switch¥ Inverse MUX all �B� channels and Data over Speech BearerSoftware/Operating Systems:¥ Supports IPX/SPX, TCP/IP, NETBIOS, Appletalk, and all other Ethernet protocols

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1381384.2.6 Communications servers, routers, bridges, multiport LAN ISDNBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

DigiBoardPC IMAC/4Multiport ISDN Network interface card/

6400 Flying Cloud Drivecommunications hub. Installs inexpansion slot of PC.

Eden Prairie, MN 55344Up to 5 cards can be installed in a singlePC

Jim Libersky1-800-344-4273

NI-1 Date:NowNI-2 Date:1994Price:1 ISDN Port $11952 ISDN Ports $19904 ISDN Ports $3980Ports1 to 4 ISDN PortsField upgradable via snap-onIDP modules

Voice Interfaces:Data Interfaces:RJ-45 (ISDN BRI)Split and combine Bchannels? Bonding? ISDN Interface:YesS/T RJ-45

Power: From Bus

Additional Features:¥ Ethernet Protocol Analyzer built in¥ Aggregates any number of channels among PC IMAC/4 cards in a PC--ideal for Multiline hunt groups¥ Fits in one standard ISA/EISA expansion slot¥ Uses both voice and/or data ISDN lines¥ Link Optimization - Reduces line charges by up to 60%¥ Field Upgradable from 1 BRI Line to 4 BRI Lines Per Card¥ MultipointSoftware/Operating Systems:¥ Novell 3.11 versions or higher¥ NetWare MultiProtocol Router¥ Windows NT (NDIS 3.0)¥ Windows Remote Access Server

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1391394.2.6 Communications servers, routers, bridges, multiport ISDN LANBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Engage Communication, Inc.Express RouterWide Area Networking for Apple Talk

9053 Soquel DriveISDN (Ethernet) & TCP/IP for Protocols

Aptos, CA 95003-4034Sync Router ISDN(Local Talk)Wide Area Networking of AppleTalkProtocols

Mark Doyle(408) 688-1021

NI-1 Date: NowNI-2 Date:Price:$1925 to $2495PortsTwo B Channels

Voice Interfaces: NoneData Interfaces: Ethernet Local TalkSplit and combine Bchannels?Yes

Bonding?Yes

ISDN Interface:S/T

Power: 24 VAC

Additional Features:¥ Icon based connectivity softwareSoftware/Operating Systems:¥ Apple Computer: Macintosh System¥ Under Development: Windows & X/Unix

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1401404.2.6 Communications servers, routers, bridges, multiport ISDN LANBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Gandalf Systems Corp.XpresswayRemote LAN Access concentrator for smalloffice and telecommuting

Cherry Hill Industrial CenterBuilding 9On demand LAN connectivity

Cherry Hill, NJ 08003

609 424-9400

NI-1 Date:NowNI-2 Date:June 94Price: Base Unit with8 BRI - $15KPorts:Up to 32 BRIUp to 4 PRI

Voice Interfaces:Data Interfaces: EthernetToken RingSplit and combine Bchannels? Yes

FDDIBonding? No

ISDN Interface:S/TPower:External

Additional Features:¥ LAN data compression up to 8:1¥ CLID, CHAP, & call back security¥ PPP protocol support¥ hot swap modules¥ optional redundancySoftware/Operating Systems:¥ supports all LAN protocols¥ SNMP management

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1411414.2.6 Communications servers, routers, bridges, multiport ISDN LANBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Hewlett Packard, Inc.HP ISDN SERVERTCP/IP Router

19410 Homestead Road- Link to Router Upgrade(J2108A)¥ concentrates workstation &

Cupertino, CA 95084Connects a TCP/IPLAN to an ISDN PC ISDN calls

HP DIRECT(800) 637-7740

NI-1 Date:NowNI-2 Date:Price:Ports1 to 3 BRIs

Voice Interfaces: N/AData Interfaces:Split and combine Bchannels?Yes- up to 384

One Ethernet(10 Base/2 or 10 Base/5)Bonding?No

ISDN Interface:S/T

Power:

Additional Features:¥ Supports full duplex transmission over up to six B channels¥ Channel allocation, dialing, call establishment and disconnection are automated and transparent to user and applications.¥ Network security provided by accepting calls only from a list of authorized callers.¥ Requires HP 9000 Series 700 and ISDN Link (J2109A) product.¥ Compatible with

OST client BRI PC products.Software/Operating Systems:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1421424.2.6 Communications servers, routers, bridges, multiport ISDN LANBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

International BusinessIBM 3174

Machines, Inc.EstablishmentController BasicAdapter card for EstabishmentCommunication Controller

Research Triangle ParkNC 27709Rate AdapterFeature #3055

Walt Reston(919) 254-0434

NI-1 Date:Not AnnouncedNI-2 Date:Not AnnouncedPrice: $5190Ports4

Voice Interfaces:Data Interfaces:Split and combine Bchannels?No

IDLC on B channelsBonding?

ISDN Interface:S/T

Power: From Bus

Additional Features:¥ Supports communication with PS/2’s equipped with one of the two Coprocessors and ISDN Coprocessor Support Program Version 1.1, Version 1.1.1 or Version 1.2.¥ Supports communication with appropriately equipped AS/400¥ Supports ISDN Data Link Control (IDLC) on B channel¥ Supports up to 8 remotes per adapter and up to 4 adapters per 3174Software/Operating Systems:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1431434.2.6 Communications servers, routers, bridges, multiport ISDN LANBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

ISDN Systems CorporationDYNA-BRIDGE

(ISC)8320 Old Courthouse Road

Suite 203Vienna, Virginia 22182

Jeff Milloy(703) 883-0933FAX: (703) 883-8043

NI-1 Date:NowNI-2 Date:Price: $2,495Ports 4

Voice Interfaces:Data Interfaces:Split and combine Bchannels?Yes

1 standard POTS (analog)LANFrame RelayBonding?ProprietaryBonding

ISDN (Basic Rate)AsyncISDN Interface:Power:2 B and D

Additional Features:The DYNA-BRIDGE“ is the ideal solution for remote LAN access and LAN to LAN interconnection.DYNA-BRIDGE may be equipped with three ISDN BRI ports for up to six simultaneous connections.Dynamic Bandwidth Allocation provides on-demand, multiple B-channel assignment for applicationsrequiring higher throughput than can be provisioned on a single channel.Software/Operating Systems:The DYNA-BRIDGE provides protocol transparency for operations in networks supporting OSI, XNS,TCP/IP, Decnet, Netware and others. Each packet is bridged or routed according to information containedin the MAC layer. The Spanning Tree Protocol provides a fault tolerant, plug-and-play solution formulti-vendor interoperability.¥ Mgmt: SNMP, ISC configurations¥ Futures: Token ring W/source routing

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1441444.2.6 Communications servers, routers, bridges, multiport ISDN LANBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

MPR Teltech LtdOB-100Communications server interfaces to

8999 Nelson WaySW 56/ISDN on the network side and toEthernet on LAN side.

Burnaby, BCCanada V5A 4B5Supports TCP/IP connectivity

(604) 293-6047FAX (604) 293-5787

NI-1 Date:Oct. 93NI-2 Date:Price:PortsPRI 1-8SW56, BRI 64/128MODEM: V.32 BIS 14.4 Kbps

Voice Interfaces: NoneData Interfaces:EthernetV. 35RS 232Split and combine Bchannels?23 B+DN x 64

Bonding?No

ISDN Interface:S/T

Power: 110v @ 15A

Additional Features:¥ LAN TCP/IP routing¥ Network modem poolSoftware/Operating Systems:¥ UNIX, SVR3

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1451454.2.6 Communications servers, routers, bridges, multiport ISDN LANBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

NCR CorporationNetwork Products DivisionPrimary Rate Interface forComten CommunicationsProcessor¥ Data Communication Controller (IBM-compatible Front End Processor)

2700 Snelling Ave. NorthSt. Paul, MN 55113-1784¥ Remote Concentrator/Processor¥ Gateway Processor

Jerry Kemp (612) 638-7828

NI-1 Date:N/ANI-2 Date:1Q94Price: $5,000 - PRI Adapter $5,000 - SoftwarePortsMultiple PRIsper system

Voice Interfaces:Not Applicable(Data Comm. Only)Data Interfaces:¥ IBM Channel¥ Micro Channel Architecture (MCA)¥ LAPD¥ SDLC for ISDNSplit and combine Bchannels?Bonding?ISDN Interface:No. 64 Kbpschannels onlyNot ApplicableDS1, S/T or U,RJ45

Power: From Comten Comm Processor

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-146146Additional Features:¥ Supports SDLC and X.25 over the B-channel.¥ Supports Automatic Bandwidth Management (add/drop B-channels based on traffic loads).¥ Will support TCP/IP over the B channel in 4Q93.¥ Supports NCP leased and switched terminal lines.¥ Supports NCP leased and switched trunk lines between Comtens, or Comtens and IBM 3745 with terminal adapter.¥ Supports CNS (a proprietary Comten trunking protocol available in addition to SNA Transmission Groups) leased trunk lines between Comten Communications Processors.¥ Will support V.110 rate adaption in 4Q93.¥ Supports Calling Party ID Security ScreeningSoftware/Operating Systems:The Comten runs under COS2 (Comten Operating System 2). The PRI Adapter runs undera UNIX-like operating system called Basic System Services 2 (BSS2).

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1471474.2.6 Communications servers, routers, bridges, multiport LAN ISDNadaptersCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Network Express, Inc.NE ISDN InterHub1. Concentrator for multiple remote LAN Adapter devices for WAN access to central LAN.

4251 Plymouth RoadAnn Arbor, MI 481052. Router

3. Bridge

Cindy Dames(313) 761-50054. Inverse Multiplexer

NI-1 Date:March 1, 1993NI-2 Date:UnknownPrice:$9,600 - $27,400PortsUp to:16 - Basic Rate lines 2 - Primary Rate lines

Voice Interfaces:Data Interfaces:V.35, RS232, Ethernet, 802.3Split and combine Bchannels?Yes, up to remotedevices capabilityto combinebandwidth.

Circuit-data Interfaces Bonding?No

Up to 32 simultaneouschannels consisting of 56and 64 Kbps ISDN Interface: Power:S/TExternal

Additional Features:¥ Calls-on Demand, Self initializing, auto answer¥ Interoperates with remote ISDN networking products¥ Consolidates multiple sites on a single primary rate ISDN line, or up to 16 Basic Rate lines at Central site.¥ Supports 56 Kbps and 64 Kbps to remote locations¥ Multi-point, multi-connection¥ Central site management of multiple incoming connections in a hunt group with a single high performance device¥ Allows multiple protocols to share access to central LAN¥ ISDN routing and bridging capabilitySoftware/Operating Systems:¥ Novell Netware¥ Banyan¥ UNIX¥ Apple¥ Windows 3.0

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-148148

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1491494.2.6 Communications servers, routers, bridges, multiport LAN ISDNBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Network Express, Inc.NE ISDN Router1. Router

4251 Plymouth RoadAnn Arbor, MI 481052. Bridge

Cindy Dames3. Inverse Multiplexer

(313) 761-5005

NI-1 Date:March 1, 1993NI-2 Date:UnknownPrice:$6,500 - $22,100PortsUp to:16 - Basic Rate lines 2 - Primary Rate lines

Voice Interfaces:Data Interfaces:V.35, RS232, Ethernet, 802.3Split and combine Bchannels?Yes, Nx64, H0(384kbps), 23B+D

Circuit-data Interfaces Bonding?No

Up to 32 simultaneouschannels consisting of 56,64, 384 Kbps. ISDN Interface: Power:S/TExternal

Additional Features:¥ Inverse Multiplexing¥ ISDN routing¥ Customer Filters¥ Calls-on Demand¥ Self initializing¥ Auto answer and Originates¥ Stores calling number information and MAC address¥ Data over speech bearer¥ Works with either 1 or 2 DNs¥ Works with custom AT&T and Northern Telecom ISDN¥ Has not been tested for NI-1 conformance¥ Multi-point, multi-connectionSoftware/Operating Systems:¥ Novell Netware¥ Banyan¥ UNIX¥ Apple¥ Windows 3.0

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-150150

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1511514.2.6 Communications servers, routers, bridges, multiport LAN ISDNBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

OST, Inc.MagellanStandalone TCP/IP Router

14225 Sullyfield CircleLAN to WAN

Chantilly, Virginia 22021

(403) 817-0400FAX: (703) 817-0402

NI-1 Date:NowNI-2 Date:Price:from $3,995Ports¥ Ethernet:10B2 or 10BT:10T2¥ WAN: 1 to 3 ISDN BRI

Voice Interfaces:N/AData Interfaces:EthernetISDN BRIX.25Split and combine Bchannels? Bonding? ISDN Interface:NoNoUp to 3 BRI

Power: stand alone unit with its own power supply

Additional Features:¥ Easy to use Windows-like user interface¥ Complete Log activity and statistics¥ SNMP agent¥ Supports connections to X.25 networks¥ Remote configurations across WAN¥ IPX routing (1Q94)Software/Operating Systems:¥ Proprietary

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1521524.2.6 Communications servers, routers, bridges, multiport LAN ISDNBridgesCOMPANY NAMEPRODUCT NAMEFUNCTIONS:

Racal-Datacom, Inc.Excalibur Network Access Communications server

1601 North Harrison ParkwayResource (ENAR)

Sunrise, FL 33323

Heather Vaughn(305) 846-6762

NI-1 Date:1Q94NI-2 Date:1994Price:PortsExpandable WAN ports2 LAN ports

Voice Interfaces:NoneData Interfaces:T-1/E-1PRIX.25EthernetToken RingSplit and combine Bchannels? Bonding? ISDN Interface:Phase 2Yes, Mode 2�U� interface

Power: External

Additional Features:¥ High end security features¥ Network management¥ Integrated X.25 PADSoftware/Operating Systems: