This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1724.2.9 Videoconferencing systems and multipoint control unitsCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

AT&TGlobal BusinessCommunications SystemsAT&TVoiceG.711/G.728G.711 (PCM) Audio Add-on

Visual CommunicationsMarket GroupMultiPoint Control Unit(MCU)Circuit-Data�Px64�

211 Mt. Airy RdBasking, Ridge, NJ 07920Contact: Linda Canulette(908) 658-6908Models:DX, FX, EX - Customer PremisesGS - Service ProviderSimultaneous activecallsUses 1 DN and SPIDor 2?24 @ 112/128 Kbps24 @ H0 (384 Kbps)

NI-1 Date:Price:Bandwidth Options:112/128 KbpsH0 (384 Kbps)

NI-2 Date:FCC Class:Bonding?

Video/Audio Coding: H.261/G.711 and G.728Multimedia Interfaces: Px64ISDN Interface:Power:PRI(AT&T, ETSI and NI-2)

Video Interfaces:NIIGs: 14NIPGs:

Additional Features:ISDN PRICascading¥ AT&T, ETSI & NI-2T1 Robbed-Bit Signaling¥ Multi-rate; (N x 64)Audio Add-On¥ H0 (384 Kbps)MCU Dial-Out¥ NFASMeet-me (dial-in)Full Px64 compliance24 VideoportsAdvanced Conferencing ModesNotification TonesVoice Activated SwitchingDynamic Trunk AllocationChair ControlDynamic Conference ResizingChoice of AC or DC powerBuilt-In 24 hour Scheduling CapabilityOptional: AT&T Conference Reservation System (PC-Based)

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1734.2.9 Videoconferencing systems and multipoint control unitsCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

AT&TTelemediaVoiceYes

Global BusinessCommunications SystemsConnection Model 70Circuit-DataTwo Channels

211 Mt. Airy RoadBasking Ridge, NJ 07920Simultaneous activecallsTwo

Taya Harmon(908) 658-7449Uses 1 DN and SPIDor 2?One

NI-1 Date:NowPrice: $6,995Bandwidth Options:112/128 Kbps

NI-2 Date:2Q94FCC Class:A, BBonding?No

Video/Audio Coding:Multimedia Interfaces: ISDN Interface: Power:BRI - S/TLocal

Video Interfaces: NTSCNIIGs:14NIPGs:

Additional Features:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1744.2.9 Videoconferencing systems and multipoint control unitsCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

Compression Labs, Inc.Cameo Personal VideoVoiceOne Channel

2860 Junction AvenueCircuit-DataOne Channel

San Jose, CA 95134David SauerhaftSimultaneous activecallsTwo

Tel: (408) 428-6759Fax: (408) 922-5429Uses 1 DN and SPIDor 2?Either

NI-1 Date:NowPrice: $2,095Bandwidth Options:BRI

NI-2 Date:FCC Class:BBonding?

Video/Audio Coding: G.711, PV2Multimedia Interfaces: ISDN Interface: Power:

Video Interfaces:NTSC,PAL, SECAMNIIGs:15NIPGs:

Additional Features:Video conferencing on a personal computerDesktop video conferencing: 15 fps, 128 x 112 pixels, color, window fully sizable by userIntegrated file snapshot, and screen transfer. High resolution mode for input of graphics.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1754.2.9 Videoconferencing systems and multipoint control unitsCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

Compression Labs, Inc.eclipseVoice

2860 Junction AvenueCircuit-DataOne or TwoChannels

San Jose, CA 95134Simultaneous activecallsTwo

Tel: 1-800-CALL-CLIFax: (408) 922-5429Uses 1 DN and SPIDor 2?Either

NI-1 Date:NowPrice:Starts at$19,900Bandwidth Options:56, 64, 112, 128

NI-2 Date:FCC Class:ABonding?

Video/Audio Coding: H.261, GTX,G.711, G.728Multimedia Interfaces: Std. Document Camera ISDN Interface: Power:S/T110V or 220V

Video Interfaces: Three Inputs,Two OutputsNIIGs:NIPGs:

Additional Features:Roll-About CartSelf-Guide User InterfacePicture-in-Picture (Moveable)Still-Frame GraphicsGraphiCam Document CameraAutofocus Pan/Tilt/Zoom CameraCamera PresetsMultipoint ReadyIntegrated ISDN or Switched 56 InterfaceOn Screen Messages with Help FunctionFull Duplex Audio with Echo CancellationOptional VCR

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1764.2.9 Videoconferencing systems and multipoint control unitsCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

DataBeam CorporationCT SeriesVoice

3191 Nicholasville RoadLexington, KY 40503(CT 250, CT 500, CT1000)Circuit-Data

Pete GammonSimultaneous activecalls

(606) 245-3500Uses 1 DN and SPIDor 2?

NI-1 Date:Price: Starting at $10,000Bandwidth Options:

NI-2 Date:FCC Class:Bonding?

Video/Audio Coding:Multimedia Interfaces: ISDN Interface: Power:

Video Interfaces:NIIGs:NIPGs:

Additional Features:DataBeam CT Series (CT 250, CT 500, CT 1000) are interactive, high resolution document conferencingsystems that transmit and display black and white or color images and text in a multipoint meeting.Text or photographic images for your conference can be scanned from a hard copy or computer generatedand imported. Users can mark-up documents using the electronic pen and white board features; all sitesreceive the modifications simultaneously in real-time and can print a hard copy within seconds.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1774.2.9 Videoconferencing systems and multipoint control unitsCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

EYETELEyeTel CommunicatorVoice

Communications, Inc.IIICircuit-Data

Ste. 206-267 West EsplanadeNorth Vancouver, BCCanada V7M 1A5Simultaneous activecalls

Tel: (604) 984-2522Fax: (604) 984-3566Uses 1 DN and SPIDor 2?

NI-1 Date:Use TAPrice:Bandwidth Options:56 Kbps to2.048 Mbps

NI-2 Date:FCC Class:Bonding?

Video/Audio Coding:H.261; NTSC or PALG.711Multimedia Interfaces: ISDN Interface: Power:

Video Interfaces:NIIGs:NIPGs:

Additional Features:Full Motion - Plus turns the PC into a video telecommunications workstation. Now, users can sendfull color, high resolution images from virtually any source (video, still camera, PC screen, etc.) toanother user’s computer screen while they are conducting a full motion video teleconference.Users can "cut and paste" documents from any Windows application, including spreadsheets, graphicsand word-processing programs, and transmit these along with other visual images. These items aretransmitted in seconds, while the full motion videoconference is simultaneously being conducted. Bothparties can "free-hand" sketch their comments (using a mouse), and make changes interactively, in realtime!

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1784.2.9 Videoconferencing systems and multipoint control unitsCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

Hitachi America LTD.CA-200VoiceSupports voice-only mode

3617 Parkway LaneNorcross, GA 30092Circuit-DataOperates in thismode for video-conferencing

Contact: Frank Banks(404) 242-1410Simultaneous activecalls2

Uses 1 DN and SPIDor 2?Yes

NI-1 Date:NowPrice: $13,900Bandwidth Options:56, 64, 112, 128

NI-2 Date:FCC Class:ABonding?No

Video/Audio Coding:CCITT H.261, G.711Multimedia Interfaces:RS-232, Audio I/O, FAX G3 ISDN Interface: Power:S/TPS2

Video Interfaces:2 RCA NTSC IN2 RCA NTSC OUTNIIGs:2,3,4,14NIPGs:

Additional Features:

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1794.2.9 Videoconferencing systems and multipoint control unitsCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

Hitachi America LTD.DP-200VoiceSupports voice-only mode

3617 Parkway LaneNorcross, GA 30092Circuit-DataOperates in thismode for video-conferencing

Simultaneous activecalls2

Contact: Frank Banks(404) 242-1410Uses 1 DN and SPIDor 2?Yes

NI-1 Date:NowPrice:$14,900Bandwidth Options:56, 64, 112, 128

NI-2 Date:FCC Class:ABonding?No

Video/Audio Coding:CCITT H.261, G.711Multimedia Interfaces:RS-232, Audio I/O, FAX G3 ISDN Interface: Power:S/TPS2

Video Interfaces:2 RCA NTSC IN2 RCA NTSC OUTNIIGs:NIPGs:None

Additional Features:Includes integrated 11" monitor

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1804.2.9 Videoconferencing systems and multipoint control unitsCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

ISCOM6103 Baltimore Avenue, 205Videoconference forISDN and SW56VoiceYes

Riverdale, MD 20737based on a PC platformCircuit-DataYes

Simultaneous activecalls2

Phone/FAX: (301) 779 - 1368Uses 1 DN and SPIDor 2?1

NI-1 Date:Nov 1992Price: $8,590 with PCincludedBandwidth Options:FST

NI-2 Date:1994FCC Class:A, BBonding?No

Video/Audio Coding:FSTMultimedia Interfaces: ISDN Interface: Power:S/TPC Bus

Video Interfaces:Two NTSCOne S-VideoNIIGs:14NIPGs:1, 6, 9, 10

Additional Features:¥ One channel for audio¥ One channel for video (ISDN or SW56)¥ International calls

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1814.2.9 Videoconferencing systems and multipoint control unitsCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

VTELDeskMaxVoice

108 Wild Basin RoadAustin, TX 78746Circuit-DataTwo Channels

1-(800) 856 - 8835Simultaneous activecallsTwo

(512) 314-2700Uses 1 DN and SPIDor 2?Either

NI-1 Date:4Q 93Price:Bandwidth Options:56 kbps-384 kbps

NI-2 Date:2Q94FCC Class:Class ABonding?Yes, with externalIMUX

Video/Audio Coding: Video - H.261 (FCIF or QCIF) Audio - G.711, G.722, G.728Multimedia Interfaces:Optional document camera ISDN Interface: Power:S/T Basic RateExternal

Video Interfaces:NIIGs: 3,4,14,15,17NIPGs:6

Additional Features:¥ Desktop 486 Computer¥ Windows user interface¥ 14 inch SVGA monitor¥ Includes high resolution, color CCD camera¥ Can participate in multiway conferences¥ Optional document cameraDeskMax Product Manager: Steve Sperle, VTEL Corp. (512) 314-2839

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1824.2.9 Videoconferencing systems and multipoint control unitsCOMPANY NAMEPRODUCT NAMECALLS SUPPORTED

Zydacron, Inc.INTERVu IIVoiceOne Channel

670 Commercial StreetManchester, NH 03101(603) 647-1000Video TeleconferencingCodecCircuit-DataSimultaneous activecallsUses 1 DN and SPIDor 2?One ChannelTwoTwo

NI-1 Date:Supports NI-1 todayPrice: $8,000.00 Includes: BRI or V.35/RS366Bandwidth Options:1 x56Kbps/64Kbps2 x56Kbps/64Kbps

NI-2 Date:1Q 1994FCC Class:ABonding?No, It is H.221compliant

Video/Audio Coding: H.261, H.221, G.711, G.722, G.728Multimedia Interfaces:1 - stereo outMCITM Digital Video API,3 - stereo in ISDN Interface: Power:S/TFrom Bus

Video Interfaces: VGA-WindowsTM overlay, or NTSC/PALNIIGs: 2,3,4,14NIPGs:None

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-183Additional Features:¥ INTERVu II board set plugs into any ISA Standard PC¥ Fully compliant with CCITT H.320, providing H.261 (P*64) full CIF (352x288 @ 15fps) video teleconferencing.¥ CCITT H.320,

H.221, H.230, H.231, H.233, H.242, H.243, H.261¥ Audio Compliance: G.711, G.722, G.725, G.728¥ Full duplex speakerphone interface with -60 db echo cancellation¥ 16 Bit color display¥ 30 fps @ QCIF 176x144¥ WindowsTM 3.1 interface¥ Resizable video window with graphic overlays on VGA/SVGA¥ API support for WindowsTM MCI (Media Control Interface)¥ High speed data transfer¥ Multimedia support: 3xvideo in NTSC/PAL, 3xAudio in stereo¥ Video output: VGA/SVGA or NTSC/PAL, Audio output: StereoWindows, MCI, are trademarks of Microsoft Corporation.