This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1834.2.10 Other ProductsCOMPANY NAMEAdtran, Inc.901 Explorer Blvd.Huntsville, AL 35806Leslie S. Conway(205) 971-8000NI-1 Compatibility NowNI-2 CompatibilityNow

PRODUCT NAMEU-BR1TEISDN Basic Rate U-InterfaceRange ExtenderEstimated Price$625

Notes:U-BR1TE - The ISDN Basic Rate U-Interface Range Extender enables the extension of theISDN �U� 2-wire interface from an ISDN PBX or switch over T-carrier lines to remote locations.Using the U-BR1TE configuration, the U interface can be deployed from the remote locationserving a maximum of 18,000 feet. The U-BR1TE plugs into an AT&T D4 channel bank, SLC-96or equivalent, or the ADTRAN BR1TE Bank.The U-BR1TE provides loopback capability for the full 2B+D, as well as individual B channels inboth the loop and carrier directions. The U-BR1TE responds to switch-based and local performancemonitoring.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1844.2.10 Other ProductsCOMPANY NAMEAdtran, Inc.901 Explorer Blvd.Huntsville, AL 35806Leslie S. Conway(205) 971-8000NI-1 CompatibilityNowNI-2 CompatibilityNow

PRODUCT NAMET-BR1TEISDN Basic Rate S/T-InterfaceRange ExtenderEstimated Price$335

Notes:T-BR1TE - The ISDN Basic Rate S/T-Interface Range Extender enables the extension of theISDN �S/T� 4-wire interface from an ISDN PBX or switch over T-carrier lines to remote locations.Using the T-BR1TE configuration, the S/T interface can be deployed from the remote locationserving a maximum of 3,000 feet, making it ideal for customer-owned networks. The T-BR1TEeliminates the need for an NT-1 by delivering the S/T interface directly to the terminal equipment.The T-BR1TE also supplies PS-1 or PS-2 power for terminal equipment. TE power is current limitedto a maximum of 12 watts for short circuit protection. The T-BR1TE plugs into an AT&T D4 channelbank, SLC-96 or equivalent, or the ADTRAN BR1TE Bank.The T-BR1TE provides front-panel loopback capability for the individual B channels in both the loopand carrier directions.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1854.2.10 Other ProductsCOMPANY NAMEAdtran, Inc.901 Explorer Blvd.Huntsville, AL 35806Leslie S. Conway(205) 971-8000NI-1 CompatibilityNowNI-2 CompatibilityNow

PRODUCT NAMEBR1/8 BR1TE BankHousing for U-BR1TE and T-BR1TErange extendersEstimated Price $1000 without common equipment $3358 with common equipment

Notes:The BR1TE Bank provides a cost-effective housing for the ADTRAn U-BR1TEs and T-BR1TEs.The BR1TE Bank is essentially a scaled-down D4 channel bank optimized for ISDN deployment.It terminates a T-carrier and can accommodate up to eight U-BR1TEs or T-BR1TEs.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1864.2.10 Other ProductsCOMPANY NAMEAdtran, Inc.901 Explorer Blvd.Huntsville, AL 35806Leslie S. Conway(205) 971-8000NI-1 Compatibility NowNI-2 CompatibilityNow

PRODUCT NAMEU-Repeater IIEstimated Price$650

Notes:The ADTRAN U-Repeater II is a mid-span device for extending the ISDN Basic Rate Interface.The U-Repeater extends the local loop to 40,000 feet of 24 AWG wire by repeating andregenerating the U-signal.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1874.2.10 Other ProductsCOMPANY NAMEAdvanced Micro Devices5204 E. Ben White Blvd.Austin, TX 78741Steve BretoiVoice: (800) 538-8450 ext 5395 or(512) 463-5395FAX: (512) 462-5101NI-1 Compatibility NowNI-2 CompatibilityNow

PRODUCT NAMEAm79C30ADigital Subscriber Controller Integrated CircuitPRICE 10K quantities, $13.60

Notes:¥ Single chip CMOS IC, integrating all features necessary to implement a 2B+D S-Interface Voice/DataTerminal Product when combined with a microcontroller subsystem. Integrates S tranceiver, LAPDprocessor, audio codec, and microprocessor and serial interfaces. Supports voice, Circuit Mode Data andPacket (B & D channel).¥ S-Interface; G-711 (POTS) compatible voice interface; non-multiplexed, iAPX microprocessor interfaceand IOM-2(TM) (ISDN Oriented Modular) serial interface.¥ Codec contains peak value registers for software based hands-free implementation.¥ Supported by TsLink3, a full ISO Layer 2/3 software package sold by TeleSoft International, (512) 282-6701. National ISDN-1 certified package currently available, as well as packages for France VN2/3,Germany ITR6, Japan INSNet64, and European NET3.¥ AMD provides full device application support. Contract (800) 538-8450 ext. 5289 or (512) 462-5289.Software and contract design services are available through TeleSoft International at (512) 282-6701.Product literature may be obtained through AMD at (800) 222-9323 or (408) 749-5703. Request documentnumbers 09893E or 12556B.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1884.2.10 Other ProductsCOMPANY NAMEAT&T Network SystemsP.O. Box 3050, 283 Schulman Blvd.Naperville, IL 60589-7050Joe Witkor: (708) 713-7108 FAX: (708) 713-7888NI-1 CompatibilityNoNI-2 CompatibilityNo

PRODUCT NAME DESTINY ACDESTIMATED PRICE

Notes:The DESTINY ACD is a CPE resident ACD supporting up to 50 agents and 50 queues. TheDESTINY ACD supports many of the features found on larger ACD�s. Features such as localqueueing with custom delay announcements; Intraflow and Interflow; statistics gathering andreporting; external Supervisor workstations and external Call Waiting/Message Displays.

ACD SYSTEM FEATURES¥ Centrex Application supporting both ¥ Trunk Group Blocking Elminated Analog and ISDN Agent instruments¥ Supervisor Costomizable Announcements¥ Optional Central Office Backup to UCD ¥ Customizable Daisy Treatments or Hunt Group¥ Link 1 Hunt Interface supporting¥ Directory Number Routing to Queue ¥ Call Monitoring¥ Agent Login ¥ Host Controlled ACD Call Routing¥ Team Intraflow ¥ Host Initiated Calling¥ Priority Queueing¥ Interflow¥ DID to Agent

MLS SYSTEM FEATURES¥ Real-Time Customer Control of ACD Resources¥ User Friendly Administration¥ Common User Interface with the PINNACLE ACD MIS¥ Real Time Color Displays¥ Agent Status Display providing:- Exception Highlighting with User Defined Thresholds- Time-In-State- Current Traffic Monitoring¥ Team Status Display- Offered Traffic with Highlighted Lost Calls- Performance by Answer Delay¥ Service Level Display- Queue Service level with Answer Delay and Abandoned Percentage¥ System Maintenance Display- Current System Status

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1894.2.10 Other ProductsCOMPANY NAMECatapult Communications Corporation180 South Whisman RoadMoutain View, CA 94041Holly Van Wart(415) 960-1025FAX: (415) 960-1029NI-1 CompatibilityNI-2 Compatibility

PRODUCT NAMEDCT-S Protocol Test SystemESTIMATED PRICEUS $50,000 - $175,000

Notes:Catapult�s DCT-S Protocol Test System, introduced in 1992, is a flexible system that iscapable of simulation, monitoring and load testing. It is the only test system that can simultaneouslytest cellular, SS7, ISDN and X.25 protocols.The key to the DCT-S system’s flexibility is its proprietary data communications programminglanguage (DCPL), which was developed specifically for protocol testing. The DCPL language allowsusers to construct multi-protocol tests exactly to their specification, and greatly simplifies the processof sending, receiving and analyzing messages.Based on a Sun SPARCstation with a powerful multi-processor architecture, the DCT-S gives users theperformance they need to generate high levels of traffic on up to 33 test ports.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1904.2.10 Other ProductsCOMPANY NAMEControlware CommunicationSystems Inc.1325 Campus ParkwayNeptune, NJ 07753Gene Litt(908) 919 - 0400NI-1 Compatibility3Q93NI-2 Compatibility1H94

PRODUCT NAMETAXI Family:ESTIMATED PRICE

IDB-64 ISDN Dial Backup Unit$3100 - $3600

SDB-56 Switched 56 Dial Backup Unit$2500 - $2800

IDB-128 ISDN Dial Backup Unit$4100 - $4500

Taxi SystemVaries based upon configuration

Notes:¥ Family of leased line backup products¥ Backup leased lines at rates up to T1/E1¥ Switched digital networking provides:Fast leased line failure backup (several seconds)Low monthly recurring chargesInternational Interworking¥ TAXI Family Intelligent Dial Backup Features:Flexible Leased Line failure detectionAutomatic Backup qualifiersAutomatic leased line restorationIncoming call securityMultirate backup (eg. 56/64 Kbps through T1/E1)Remote management and SNMP supportFull interworking in over 16 countries

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1914.2.10 Other ProductsCOMPANY NAMEDGM&S, Inc.1025 Briggs Rd., Suite100Mt. Laurel, NJ 08054(609) 866-1212Dan Davidson(216) 494-7773NI-1 CompatibilityNowNI-2 Compatibility12/93

PRODUCT NAMEQFax Group 4 FacsimileESTIMATED PRICECall for pricing

Notes: QFax is a recent addition to the QSourceTM family of Enabling Technology products. QFaxprovides telecommunications developers, system integrators, and service providers with a portablesoftware package that implements Group 4 digital facsimile standards defined by CCITT for theISDN.The QFax software consists of a Session and Transport Layer running above the existingQSourceTM X.25 Network Layer software. Layers 1-5 of the CCITT protocol stack are implementedon the PC/AT communications co-processor. An Application Programmer Library (API) is providedon the host platform as a callable C library.All software is written in ANSI C for ease of portability and maintenance. DGM&S provides allnecessary Q.931 signalling functions for end-to-end negotiation of the G4 bearer capability prior toactual connection of the ISDN call.DGM&S offers a low cost ISDN Multimedia Development Card (IDC-31) for the PC/AT thatsupports the Group 4 standard. The IDC-31 supports simultaneous data, voice, and analogmodem/fax emulation on a single DSP processor. For example, two simultaneous Group 4 faxtransmissions are supported on two B Channels at rates up to 64 Kbps. The IDC also supportsmixed mode operations such as V.22bis modem emulation and Group 4 fax. Future plans includeintegration of commercial Group 3 Fax and V.32bis modem packages (3/94).

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1924.2.10 Other ProductsCOMPANY NAMEGammaLink1314 Chesapeake TerraceSunnyvale, CA 94804(408) 744 - 1400FAX (408) 744 - 1900NI-1 CompatibilityYes, withadapterNI-2 CompatibilityYes, withadapter

PRODUCT NAMEGammaFax MLCP4-MVIPFour Port FAX cardESTIMATED PRICE$3395

Notes:The MLCP4-MVIP is a four port group 3 FAX card suitable for use with any of the primary rate MVIPmultiplexor cards. Primary rate solutions incorporating 23 lines of G3 FAX in a single PC chassis arepossible, with mixed voice, data, and FAX resources running on the MVIP PCM bus.Sales Contact:Robert Green, Director North American Sales(408) 745 - 2202Technical Contact:H.S. Magnuski, Chief Technical Office(408) 745 - 2275

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1934.2.10 Other ProductsCOMPANY NAMEHarris/Dracon809 Calle PlanoCamarillo, CA 93012John Onnen(805) 987-9511NI-1 CompatibilityNowNI-2 Compatibility

PRODUCT NAMEbiTS-1“ Test Set S/T Interface ISDN Interface BRI test setESTIMATED PRICE List Price: $695.95

Notes:¥ Verifies presence of 1.430 physical layer frames.¥ Supports either passive bus or point to point.¥ Supports scrambled audio monitoring of line activity.biTS-1 is a trademark of Harris Corporation.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1944.2.10 Other ProductsCOMPANY NAMEMitel CorporationCommunicating ObjectsP.O. Box 13089360 Legget DriveKanata, Ontario, Canada K2K 1X3(613) 592-2122FAX: (613) 592-4784NI-1 CompatibilityNI-2 Compatibility

PRODUCT NAMEMVIP Prototype Card(MB89020)ESTIMATED PRICE$795

Notes:The MVIP Prototype Card is a standard platform to allow rapid prototyping of design configurationsprior to committing to full board layout. This card can be used to debug or fine tune the design, or topermit software development to proceed prior to production hardware availability, thereby decreasingthe end product�s time to market. It can also be used to support small volume production applications,where design of a dedicated board would not be economical.The MB89020 contains 16 square inches of prototype (wire wrap) area. It has a standard PC businterface, along with a 256-channel digital switch and a digital telephone chip to provide an analoginterface. The MVIP expansion header allows for the card to be quickly integrated with other MVIPboards.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1954.2.10 Other ProductsCOMPANY NAMEMitel CorporationCommunicating ObjectsP.O. Box 13089360 Legget DriveKanata, Ontario, Canada K2K 1X3(613) 592-2122FAX: (613) 592-4784NI-1 CompatibilityNI-2 Compatibility

PRODUCT NAMEISDN Express Development System(MB89000)ESTIMATED PRICE$1,800

Notes:The ISDN EXPRESS Development System is a family of PC cards and supporting software which canbe used to easily evaluate Mitel Semiconductor�s ST-BUS family of digital components, as well as toquickly prototype typical communications systems. The cornerstone of the family is the MB89000CISDN EXPRESS Card. It contains a range of Primary Rate and Basic Rate interfaces, digital phonecomponents, all interconnected by a 256 channel digital switch.All of the cards are linked together by the MVIP compatible expansion header, as well as by the ISDNEXPRESS Evaluation System (IES) software. The IES software permits both cards to be linkedtogether as if they were one.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1964.2.10 Other ProductsCOMPANY NAMEMPR Teltech Ltd.8999 Nelson WayBurnaby, BCCanada V5A 4B5(604) 293-6047FAX: (604) 293-5787NI-1 CompatibilityOct ’93NI-2 Compatibility

PRODUCT NAMEHQA 100/200 Audio Encoder/DecoderESTIMATED PRICE

Notes:¥ Encodes/decodes high quality audio (24Khz) for transmission over ISDN or SW56¥ I50 MPEG Layer II compatible¥ Networked broadcast applications for collection, program generation and transmission¥ Contains inverse mux/demux functionality (4-SW56 or 3 ISDN), H.221 compatible.¥ ISDN & SW56 Network interfaces.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1974.2.10 Other ProductsCOMPANY NAMENational Semiconductor Corp.2900 Semiconductor DriveSanta Clara, CA 95052-8090Call: Frank Stempski(408) 721-7000Or National Semiconductor’s Customer Response Center1-800-272-9959 (US)1-800-258-6768 (Canada)NI-1 CompatibilitySee notesNI-2 CompatibilitySee notes

PRODUCT NAMEisoENET hub chipsetisoENET node (PC) chipsetESTIMATED PRICEOn request

Notes:The above products to be announced during 1994. Contact NSC for release dates and technical data.NI-1/2 compatibility to be determined by hub/PBX vendors.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1984.2.10 Other ProductsCOMPANY NAMENational Semiconductor Corp.2900 Semiconductor DriveSanta Clara, CA 95052-8090Bob Erickson(408) 721-4392NI-1 CompatibilityNowNI-2 CompatibilityNow

PRODUCT NAMETP3410 - 2B1Q U Interface TransceiverBasic Rate Access Integrated CircuitTP3420A - S/T Interface TransceiverBasic Rate Access Integrated CircuitESTIMATED PRICEOn request

Notes:¥The TP3410 is a complete single chip CMOS transceiver for ISDN Basic Access at either end of theU interface. It provides full duplex transmission at 160 kbps over a single twisted pair via a simpletransformer interface circuit. The range exceeds 18 Kft of #24 AWG (1300 ohm loops).¥Complies with ANSI T1.601 US Standard¥Product support includes the TP3410 Datasheet, Users Manual and Evaluation Board.¥The TP3420A is a complete single chip CMOS transceiver for ISDN Basic Access at eitherend of the S/T interface. It provides full duplex transmission over separate transmit and receivetwisted pairs up to 1.5 km.¥Complies with ANSI T1.605 and CCITT I.431 Standards.¥Product literature consists of the TP3420A datasheet and Application Note AN665: S InterfaceDevice Users’ Guide.¥Product literature may be obtained through the customer response center at 1-800-272-9959 in theUS, or 1-800-258-6768 in Canada.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-1994.2.10 Other ProductsCOMPANY NAMENetwork Communications Corp5501 Green Valley DriveBloomington, MN 55437-1085Stephen Stange(612) 844 - 0584NI-1 CompatibilityNowNI-2 Compatibility1/94

PRODUCT NAME NP7050I ISDN TesterESTIMATED PRICE10,900

Notes:The NP7050I can monitor and emulate BRI, PRI, V.120, LAPD/X.25, Q.921/Q.931 at the �S�, �T�,and �U� interfaces, and includes VT220 terminal emulation, BERT, Digital TIMS, and remote control.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-2004.2.10 Other ProductsCOMPANY NAMENetwork Communications Corp5501 Green Valley DriveBloomington, MN 55437-1085Stephen Stange(612) 844 - 0584NI-1 CompatibilityNowNI-2 Compatibility1/94

PRODUCT NAMENP7050P Primary RateISDN TesterESTIMATED PRICE$9600

Notes:The NP7050P can monitor and emulate PRI, V.120, LAPD/X.25, Q.921/Q.931 at the �S�, �T�, and �U�Primary Rate Interfaces, and includes VT220 terminal emulation, BERT, Digital TIMS, and remotecontrol.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-2014.2.10 Other ProductsCOMPANY NAMENetwork Communications Corp5501 Green Valley DriveBloomington, MN 55437-1085Stephen Stange(612) 844 - 0584NI-1 CompatibilityNowNI-2 Compatibility

PRODUCT NAME NP7050BESTIMATED PRICE$9800

Notes:The NP7050B can monitor and emulate BRI, V.120, LAPD/X.25, Q.921/Q.931 at the �S�, �T�, and �U�Basic Rate interfaces, and includes VT220 terminal emulation, BERT, Digital TIMS, and remote control.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-2024.2.10 Other ProductsCOMPANY NAMENetwork Communications Corp5501 Green Valley DriveBloomington, MN 55437-1085Stephen Stange(612) 844 - 0584NI-1 CompatibilityNowNI-2 Compatibility1/94

PRODUCT NAME NP7100I ISDN TesterESTIMATED PRICE$14,995

Notes:The NP7100I can monitor and emulate BRI, PRI, V.120, LAPD/X.25, Q.921/Q.931 at the �S�, �T�, and �U�interfaces, and includes VT220 terminal emulation, BERT, Digital TIMS, remote control, data linemonitor, lead status, speaker monitor, DVOM/Tone Generation, and Digital Oscilloscope.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-2034.2.10 Other ProductsCOMPANY NAMENitech, Inc.(New Information Technologies, Inc.)4400 Route 9 SouthFreehold, New Jersey 07728Dilip GuhaTel. (908) 303-7471NI-1 CompatibilityYesNI-2 Compatibility1994

PRODUCT NAMENitelOwl1010 Test SetNiteOwl 1230 Test SetNiteOwl 1320 Test SetNiteOwl 1630 Test SetESTIMATED PRICE$10,000$14,000$15,000$19,000

Notes:¥ NiteOwl Series Test Set can monitor and simulate BRI, PRI, V.35/RS-232, LAPD/X.25, Q.921/Q.931 at S/T, PRI/T-1 and V.35/RS-232 interfaces.¥ NiteOwl Series support fractional T-1 up to 2.048 Mbps¥ NiteOwl Series simulate and monitor all 24/31 Channels simultaneously¥ NiteOwl Series can run BERT testing on T-1 line including monitoring and simulation of ESF data link and Robbed Bit Signaling¥ NiteOwl Series can support ATM, SMDS, Frame Relay Protocol in monitor and simulation mode

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-2044.2.10 Other ProductsCOMPANY NAMEObertronics Software Inc.P.O. Box 279North Reading, MA 01864Daniel K. O�Brien(508) 664 - 2205FAX (508) 664 - 2205NI-1 CompatibilityNowNI-2 Compatibility

PRODUCT NAMEISDN Message Desk (C)ESTIMATED PRICE $2500 / Position

Notes:The ISDN Message Desk is a completely integrated software and hardware application package thatprovides ISDN Call Coverage Services, including MHS Electronic Mail Access Services, Pink SlipFront Desk Operations, Help Desk Directory Look-Up Services, Automatic Call Wake-up andScheduling Service (for Hotel/Motel or College Campus type service). Client/Remote calendarsfor individual schedules. The application can be utilized in all work environments, ranging fromsmall team size and/or departmental groups, to large company-wide centered operation.Additional Features include:¥ Automatic Installation Programs¥ Message Archiving to Hard Drives¥ Bulk Database Up-Loading and Down Loading to floppy drives, or via mainframes¥ Security access codes¥ Client Account Billing System¥ Attendant Traffic Reports, CSS, Call Count, Holding Times, etc., Group/Individual Reports¥ Supervisor/Client Access to LAN Calendaring ModulesMS DOS, PCDOS, and Netware CompatibleISDN Message Desk is a copyright of Obertronics

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-2054.2.10 Other ProductsCOMPANY NAMESiemens Stromberg-Carlson900 Broken Sound Parkway NWBoca Raton, FL 33487Jim Wood(407) 955-8354NI-1 CompatibilityNowNI-2 CompatibilityNow

PRODUCT NAME91469 ISDN Basic Rate Interface(BRIU) Channel UnitBasic Rate U Interface Distance ExtenderESTIMATED PRICE

Notes:This Channel Unit provides transport of ISDN Basic Rate (2B+1D) information overT1 spans. It can deliver ISDN service to customers from a distant ISDN switch inthose instances where the serving central office is not ISDN capable.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-2064.2.10 Other ProductsCOMPANY NAMETeloquent Communications Corp.4 Federal StreetBillerica, MA 01821-3594(508) 663-7570FAX: (508) 663-7543NI-1 CompatibilityNowNI-2 CompatibilityYes, when documented

PRODUCT NAMEDistributed Call CenterESTIMATED PRICE $2500/per user

Notes:Distributed Call Center is an advanced automatic call distribution (ACD) system implemented insoftware on commodity PC�s. Using ISDN BRI as an access mechanism, it empowers users to leveragethe ubiquity and power of the public telephone network, giving them freedom to place call center agents(customer service representatives) anywhere, including headquarters, branch offices, or working athome. Agent phone options include a high-function ISDN set, or the �telephone� can be a MicrosoftWindows application running in a PC equipped with an ISDN adapter, which through WindowsDynamic Data Exchange (DDE), facilitates Computer-Telephone Integration (CTI) independent of thehost computer and/or data network. The system provides advanced ACD features - tightly integratedwith voice and information processing - without proprietary, customer premises switches.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-2074.2.10 Other ProductsCOMPANY NAMETrillium Digital Systems, Inc.2001 S. Barrington Ave., # 215Los Angeles, CA 90025Phone: (310) 479-0500FAX: (310) 575-0172NI-1 CompatibilityYesNI-2 CompatibilityUnder development

PRODUCT NAMEQ.930/Q.931 Portable Source CodeESTIMATED PRICEQ.930/Q.931 User Side $20,000Q.930/Q.931 Network Side $20,000Q.930/Q.931 User & Network $36,000Q.930/Q/931 NI-1 Variant $ 4,000

Notes:Trillium develops and markets communications software including X.25, Frame Relay, SS7,Q.930/931, and Q. 93BOur Q.930/Q.931 portable source code is available in ten variants currently. Other Trilliumproducts that are typically used in conjunction with Q.930/Q/931 include LAPB, LAPD, X.25and X.31.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-2084.2.10 Other ProductsCOMPANY NAMEVeriFone9040 Roswell RoadAtlanta, GA 30350John Menzel(404) 552-3448NI-1 CompatibilityWith TANI-2 CompatibilityWith TA

PRODUCT NAMEOmni POS TerminalTranz POS TerminalESTIMATED PRICE$300 - 400$500 - 600

Notes:VeriFone manufacturers POS Terminals for credit card, debit card, and check authorizations andsettlement. The POS Terminal can be integrated with an Electronic cash register or stand alone.Both the Omni and Tranz line of POS Terminals interface to ISDN Terminal Adapters. The Omniand Tranz terminals support the T3POS protocol. The Omni line also comes in a LAN configurationwith the LAN Controller interfacing to the ISDN TA.

This information is subject to change without notice.See Notice of Disclaimer on Title Page4-2094.2.10 Other ProductsCOMPANY NAMEVeriFone9040 Roswell RoadAtlanta, GA 30350John Menzel(404) 552-3448NI-1 CompatibilityWith TANI-2 CompatibilityWith TA

PRODUCT NAME Emerald Transaction Super SystemESTIMATED PRICE $700 - 1,000

Notes:The Emerald Product Line is used in the healthcare industry. The Emerald allows electronicsubmission of claim forms. It eliminates the need for manual submission of forms, greatly speedingup the accuracy of claims and time to re-imbursement. The Emerald interfaces to ISDN TAs andsupports the T3POS protocol.