˚This information is subject to change without noticeSee Advisory Note on Title Page8-18.List of AcronymsACDAutomatic Call DistributionAMAAutomatic Message AccountingANIAutomatic Number IdentificationANSIAmerican National Standards InstituteB (Channel)A 64 kbps digital information channelbpsBits per secondBRIBasic Rate InterfaceCACall AppearanceCCITTConsultative Committee for International Telegraphy and TelephonyCFDACall Forwarding Don’t AnswerCICCarrier Identification CodeCLAMNCall Forwarding Address Modified NotificationCLIDCalling Line IdentificationCMDCircuit-mode-dataCNDCalling Number DeliveryCPECustomer-premises-equipmentCRCall ReferenceCSU/DSUChannel Service Unit/Data Service UnitDLCIData Link Connection IdentifierDMADirect Memory AccessDMSDigital Multiplex SwitchingDNDirectory Number

This information is subject to change without noticeSee Advisory Note on Title Page8-2DNICData Network Identification CodeDNSData Network SystemDSMDemand Side ManagementDSPDisplay Station ProtocolEIDEndpoint IdentifierEKTSElectronic Key Telephone ServiceESSElectronic Switching SystemFAXFacsimileFEPFront End ProcessorFTPFile Transfer ProtocolFXForeign ExchangeHLCHigh Layer CompatibilityIDIdentificationIECInterExchange CarrierIMUXInverse MultiplexerINICISDN Network Identification CodeIOFInter Office FacilityISDNIntegrated Services Digital NetworkISOInternational Standardization OrganizationITU-TSSInternational Telecommunications Union - TelecommunicationsStandardization Section (formerly, CCITT)JPEGJoint Photographic Experts GroupkbpsKilobits per secondkHzKilohertzLANLocal Area Network

˚This information is subject to change without noticeSee Advisory Note on Title Page8-3LATALocal Access and Transport AreaLCLogical ChannelLECLocal Exchange CarrierLLCLogical Link Control (LAN)LLCLow Layer Compatibility (ISDN)MACMedium Access ControlMbpsMegabits per secondMFMulti-Frequency SignalingMLHGMultiline Hunt GroupMPEGMoving Pictures Experts GroupMR CMDMulti-rate Circuit Mode DataNI-1National ISDN-1NI-2National ISDN-2NIIGNIUF ISDN Interface GroupNIPGNIUF ISDN Parameter GroupNISTNational Institute of Standards and TechnologyNIUFNorth American ISDN Users’ ForumNTNetwork TerminationNTSCNational Television System CommitteeNUINetwork User IdentificationOSI Open Systems InterconnectionPBXPrivate Branch ExchangePCPersonal ComputerPHFPacket Handling FunctionPMDPacket-Mode Data

This information is subject to change without noticeSee Advisory Note on Title Page8-4POTSPlain Old Telephone ServicePPSNPublic Packet Switched NetworkPRIPrimary Rate InterfacePSTNPublic Switched Telephone NetworkPVCPermanent Virtual CircuitRGBRed-green-blue (monitor)SFGStimulated Facility GroupSPCSStored Program Controlled Switching SystemSPIDService Profile IdentifierSS7Signaling System 7SWF-DS1Switched DS1/Switched Fractional DS1 Service CapabilityT3 POSTransaction Processing Protocol for Point-of-SaleTATerminal AdapterTCP/IPTransport Control Protocol/Internet ProtocolTETerminal EquipmentTEITerminal Endpoint IdentifierTSPTerminal Service ProfileUDIUnrestricted Digital InformationUUIUser-to-User InformationVMSVoice Messaging System